Allgood Ltd, 63-83 Brearley Street,Hockley,Birmingham,B19 3NT



**Office:** 0121 359 4415

**Specification Sales Representative:** Ivana Kubicova

**Mobile:**

**Email:** ivana.kubicova@allgood.co.uk

**Estimator:** Samir Hassaine

**Email:** samir.hassaine@allgood.co.uk

**Project: Museum of London, Smithfield (MP)**

**Schedule: Q00029298\_07 Poultry Market - Ironmongery - Raphel Timber Doors**

**Latest Document Details**

This specification has been produced using our best skill and judgement and is based on the documents provided to us, bearing the following references, from which all relevant details have been taken.

Floor Plans

2125-SWA-PM-B1-DR-A-32200 rev P01 dated 16/12/2020

2125-SWA-PM-BM-DR-A-32201 rev P01 dated 16/12/2020

2125-SWA-PM-00-DR-A-32202 rev P01 dated 16/12/2020

2125-SWA-PM-01-DR-A-32203 rev P01 dated 16/12/2020

Door Elevations

2125-SWA-PM-XX-DR-A-32601 rev P01 dated 23/12/2020

2125-SWA-PM-XX-DR-A-32602 rev P01 dated 23/12/2020

2125-SWA-32603 rev -

2125-SWA-32604 rev -

Door Schedules

2125-SWA-PM-B1-DR-A-32901 rev -

2125-SWA-PM-B1-DR-A-32902 rev -

2125-SWA-PM-BM-DR-A-32903 rev -

2125-SWA-PM-00-DR-A-32904 rev -

2125-SWA-PM-00-DR-A-32905 rev -

2125-SWA-PM-01-DR-A-32906 rev -

2125-SWA-PM-01-DR-A-32907 rev -

Typical Door Detail

2125-SWA-DR-A-32670 rev -

No door elevations for glazed doors provided.

Allgood Schedule Q00029298\_02 compiled from A Hogger mail instruction 31/03/21 at 21:51 hours along with annotation of Allgood Schedule Q00029298\_01

2125 SWA PM XX DR A 32601 Rev T01 S4 dated 14/12/2020

2125 SWA PM XX DR A 32602 Rev T01 S4 dated 14/12/2020

Q00029298\_04 has been compiled to the below documents ;

Door Schedule : 2125-SWA-PM-XX-SH-A-32901 - 22/12/2023 EWN0093 clarifications - EWN0415 & EWN0419 C01

Marked Up Floor Plans - 508\_SK\_ 2548 \_ Rev B - EW 123 - PM Review of internal doors - 06 / 03 / 2024

Q00029298\_05 - Price Update

Q00029298\_06 - Price Update

Q00029298\_07 has been compiled to the below documents ;

Door Schedule : 2125-SWA-PM-XX-SH-A-32901 - 22/12/2023 EWN0093 clarifications - EWN0415 & EWN0419 C01

Marked Up Floor Plans - 508\_SK\_ 2548 \_ Rev B - EW 123 - PM Review of internal doors - 06 / 03 / 2024

**Technical Notes**

All items are supplied, unless otherwise indicated, complete with fixings suitable for timber.

We have allowed for intumescent packs for hinges, lock cases and flush bolts to fire rated doors.

Please note that these are essential for the fire performance of our products and are tested as a working set. Should you require these to be removed, separate provision will need to be made and clarification sought as to the suitability of such provision (by a certified third party).

**Remarks**

Please see the remarks section of each set for any questions relating to this specification that need answering prior to any order being placed.

Wall Readers, RTU buttons/pads, Break glass units and access control for further discussion with Allgood Secure.

We have assumed door thickness to be 44mm unless told to the contrary.

**Other Details Required**

Kicking plate sizes are nominal sizes only, confirmation of the exact sizes will be required from the contractor prior to manufacture.

Details of the master key suiting are required. Please note that provision can be built into the master key system easily at the time of ordering to accommodate any possible future extensions to the suite. It is however difficult, if not impossible, to greatly extend the master key suite if approximate requirements have not been clarified before manufacture. Please understand that the master/sub master keys will only be released upon receipt of a letter of authorisation from the architect or client. Please confirm the quantity of each master and sub master key required for which there is an additional charge.

Please note, we have priced for master keying based on a new and unique suite. Should the project require suited cylinders as part of an extension to an existing suit, additional costs may be incurred based upon suite type.

If alternative and non-Allgood cylinders are being sourced, the manufacturer and cylinder type will need to be confirmed as well as a sample issued to ensure compatibility with Allgood lock cases.

**General Conditions**

"Please note that all orders and customer call-offs under £750 will be subject to a £15 carriage charge.

Order and customer call-offs over £750 will be free of charge, however this only allows for an ""anytime next day"" delivery and not a specific timed slot nor any non-standard delivery requirements. (These are available on request and at an extra charge depending upon requirements)."

Items marked with an '\*' will be produced/manufactured specifically for this project and are non-returnable. Due to these being non stock items the lead times from the time you place your order with us are likely to be a minimum of four weeks but lead times do vary from item to item. Please contact us for further details if required.

Please note, unless otherwise stated this quotation/schedule does not allow for any provision of control samples or sample boards. These are available at an additional cost dependent upon the project requirements, please contact your Allgood Sales Representative or your local Allgood office for more details.

This document, the specifications and the schedules that are contained herein are the copyright of Allgood. It has been produced for the sole use of the project team and no licence is implied or given for their dissemination or distribution to any other parties without our express prior consent in writing. Relaxation is available as described in section 17 of our standard Terms and Conditions.

Many products described in this schedule are protected by copyright and design registration. By describing and illustrating them we are not providing or implying any licence to third parties to offer copies of them.

This schedule is subject to our standard Terms and Conditions which are attached.

This schedule is open for acceptance for a period of 90 days from the date of issue. Prices are fixed for all deliveries made within a period of 90 days from the date of acceptance and are subject to value added tax at the rate applicable on the date of despatch. We reserve the right to requote these prices at the end of the above fixed price period.

Please note that the attached schedule does not allow for door by door packaging. Although this service is available from Allgood there is a charge for its provision based on the contract value. In our experience project managers prefer pre-morticed items to be delivered directly to the door manufacturers and the remaining hardware delivered directly to site. Please also note that extra large items such as kick plates and long pull handles as well as master keyed cylinders would not appear in the door by door packages. For further details please contact your sales representatives quoting the project name as stated on this schedule.

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 01 -** | **BOH - Double - DRT-01 - BWD/02/05/a/FD60/AC** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 8.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 16.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | XX97948SS | Allgood Alite® FDKLS 76øx1.2mm 'Fire Door Keep Locked Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | SS48800F | Allgood Hardware 203x19x11mm Lever Action Flush bolt, with coil spring, parallel movement radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48800FP] |
| 1.00 ea | SS48801F | Allgood Hardware 457x19mm Lever Action Flush bolt, with coil spring, parallel movement, radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48801FP] |
| 1.00 ea | SS7051 | Allgood Hardware 63x20x38mm easi-clean socket for wood or stone, grade 316, satin stainless finish |
| 1.00 ea | XX48800FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48800 flush bolts |
| 1.00 ea | XX48801FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48801 flush bolts |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 2.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |
| 1.00 ea | XX75574 | Allgood Secure 270x52x28mm surface mounted architectural electromagnet and armature for use on single door applications, 300kg holding force, MBS monitored and dual 12/24 DC voltage with 250ma current draw @ 12 volts and 125ma current draw @ 24 volts, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 60 minutes on metal doors |
| 1.00 ea | XX75574ZLC \* | Allgood Secure Z and L bracket armature assembly complete with architectural cover for use with XX75574 electromagnet. For use on inward opening doors only. |
| 1.00 ea | XX90009 \* | Access control to be supplied by others |

|  |
| --- |
| Total GBP: 978.52 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.39.01 | PM.DR.B1.52.01 | PM.DR.B1.PL07.01 |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| We have assumed doors have plain meeting stiles. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 0104 -** | **FOH - Single cleaners cupboard (FD30) - Surface Closer - DRT-02a - CL** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 3.00 ea | SS8066R | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with radius corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 3.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SN7319BM \* | Allgood Hardware 'B' 70mm (35/35) length Euro Profile Cylinder & turn, independently tested to BS EN 1303:2015 classification 1/6/0/B\*1/0/C/6/D, trademark protection 6 pin cylinder with solid and lateral profile pins, c/w “anti-Bump”, “anti-pick”, “anti-drill” and “anti-pull” protection, 2 keyed, under master key, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors, satin nickel plated finish |
| 1.00 ea | SS7286F60 | Allgood Hardware 92x60mm backset HL series profile cylinder mortice deadlock case only, single throw 20mm Stainless Steel deadbolt, rounded forend & strike CE Marked to BS EN: 12209 3/X/8/1/0/G/2/B/A/0/0 Certifire approved CF347 for use on 90 minute timber fire doors and up to 240 minutes for metal fire doors, 10 year manufacturing warranty, satin stainless steel finish |
| 1.00 ea | XX7286FP6 | Allgood Hardware intumescent Lock Fire Pack 7286 60mm backset Series |
| 2.00 ea | SS796Q | Allgood Modric® 50x4mm Circular Escutcheon for Euro Profile Cylinder, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and for up to 240 minutes on metal doors, grade 316, 25 year manufacturing warranty, satin stainless steel finish |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 2.00 ea | SS8449 | Allgood Hardware 76mm circular 'Fire door keep shut' symbol, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, satin stainless steel finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | SS2301 | Allgood Hardware 38x47mm Heavy Duty Circular Floor Mounted Door Stop, grade 316, 25 year manufacturing warranty, satin stainless steel finish |
| 1.00 ea | SS8455 \* | Allgood Modric® 76ømmx2.5mm 'Cleaners - Mop & Bucket graphic' sign with torx screw fixings, satin stainless steel finish |

|  |
| --- |
| Total GBP: 392.96 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.01.57.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 0105 -** | **FOH - Single circulation door (FD30) 2.2 - nds - DRT-34** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 3.00 ea | SS8066R | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with radius corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 3.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SS1761 | Allgood Mode® 700x67x19mm entrance pull handle with bolt through fixings at 600mm centres, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | SS8449 | Allgood Hardware 76mm circular 'Fire door keep shut' symbol, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, satin stainless steel finish |

|  |
| --- |
| Total GBP: 245.39 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.01.28.02 | PM.DR.01.53.01 | PM.DR.01.54.02 |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| Is locking required? |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 0106 -** | **FOH - Single lockable circulation door (FD) 2.2 - wds - DRT-34 - FWD/01/06/c/FD30a** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 3.00 ea | SS8066R | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with radius corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 3.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SS1761 | Allgood Mode® 700x67x19mm entrance pull handle with bolt through fixings at 600mm centres, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | SS2301 | Allgood Hardware 38x47mm Heavy Duty Circular Floor Mounted Door Stop, grade 316, 25 year manufacturing warranty, satin stainless steel finish |
| 2.00 ea | SS8449 | Allgood Hardware 76mm circular 'Fire door keep shut' symbol, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, satin stainless steel finish |

|  |
| --- |
| Total GBP: 259.56 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.01.62.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| Is locking required? |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 0107 -** | **FOH - Single door - DRT-35 - FWD/15/06/c/FD60/AC/EHO** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 6.00 ea | SS8066R | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with radius corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 1.00 ea | XX9133FPNE \* | Allgood Hardware Size 2-4 Concealed Emag Cam Closer Intumescent Pack for use on up to 60 minute timber fire doors to suit 9133NE |
| 1.00 ea | SN9133NE \* | Allgood Hardware 280x46x33mm Concealed Overhead Electrical Hold-open Door Closer, complete with finished track and arm for Single Action Doors, adjustable power '3-4', closing force, latch action, Certifire approved CF6022 & CE Marked to BS EN 1155: 3-8-4/3-1-1-3, 10 year manufacturer warranty, SNP finish |
| 12.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | SS1763N \* | Allgood Mode® 1300x67x19mm entrance pull handle with bolt through fixings at 1200mm centres for doors 35-54mm thickness, grade 316, satin stainless finish |
| 2.00 ea | SS8447 | Allgood Hardware 76mm circular 'Automatic fire door keep clear' symbol, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, satin stainless steel finish |
| 2.00 ea | SS8448 | Allgood Hardware 76mm circular 'Fire door keep locked' symbol, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, satin stainless steel finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | SS48800F | Allgood Hardware 203x19x11mm Lever Action Flush bolt, with coil spring, parallel movement radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48800FP] |
| 1.00 ea | SS7051 | Allgood Hardware 63x20x38mm easi-clean socket for wood or stone, grade 316, satin stainless finish |
| 2.00 ea | XX48800FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48800 flush bolts |
| 1.00 ea | XX75574 | Allgood Secure 270x52x28mm surface mounted architectural electromagnet and armature for use on single door applications, 300kg holding force, MBS monitored and dual 12/24 DC voltage with 250ma current draw @ 12 volts and 125ma current draw @ 24 volts, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 60 minutes on metal doors |
| 1.00 ea | XX75574ZLC \* | Allgood Secure Z and L bracket armature assembly complete with architectural cover for use with XX75574 electromagnet. For use on inward opening doors only. |
| 1.00 ea | XX90010 \* | See Remarks |
| 1.00 ea | SS2301 | Allgood Hardware 38x47mm Heavy Duty Circular Floor Mounted Door Stop, grade 316, 25 year manufacturing warranty, satin stainless steel finish |
| 1.00 ea | XX90009 \* | Access control to be supplied by others |

|  |
| --- |
| Total GBP: 924.26 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.01.46.01 | PM.DR.01.47.01 |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| Assumme Doors to have plain meeting stiles.  PSU in sundries set. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 0108 -** | **BOH - Double door - DRT-01 - BWD/02/05/a/EHO/FD30/AC - BLA** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 8.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 8.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 2.00 ea | XX98141S66 | Allgood Hardware, Figure 6, soffit bracket & template, satin stainless steel finish |
| 2.00 ea | XX98181S6 | Allgood Hardware Surface Mounted Electromagnetic Hold Open Overhead Door Closer, with swing free option, controlled closing, power size 4, universal fixings for timber and metal doors, supplied c/w black power transfer loop, frame mounted connection box and on/off switch, Certifire CF5517 listed to BS EN 1155, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on insulated metal doors, 10 year manufacturer warranty, satin stainless steel finish |
| 2.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | XX75574D \* | Allgood Secure 520x52x28mm Surface Mounted Architectural Electromagnet and Armature, for use on double door applications, 300kg holding force (on each door leaf), MBS monitored and dual 12/24 DC voltage, with 500ma current draw @ 12 volts and 250ma current draw @ 24 volts, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 60 minutes on metal doors |
| 2.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | XX75574DZLC \* | Allgood Secure Z and L bracket armature assembly complete with architectural cover for use with XX75574D electromagnet. For use on inward opening doors only, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 60 minutes on metal doors |
| 4.00 ea | XX97947SS | Allgood Alite® ADFKC 76øx1.2mm 'Automatic Fire Door Keep Clear' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 2.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |
| 2.00 ea | ZQ0062599 \* | Allgood Hardware 55x400x1.5mm Satin Stainless Steel Frame Protection Plate. Undrilled - SELF ADHESIVE BY OTHERS  NOMINAL SIZE ONLY - EXACT SIZES TBC FROM SITE |
| 1.00 ea | XX90009 \* | Access control to be supplied by others |

|  |
| --- |
| Total GBP: 1,727.21 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.58.04 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| We have assumed doors have plain meeting stiles.  PSU in sundries set |  |  |  |
| Make up of frame protection plate to be confirmed. Offcuts of tread plate to be considered. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 0109 -** | **FOH - Leaf & half - Shared Equipment Space MECH/HO - DRT-35 - NFD** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 6.00 ea | SS8066R | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with radius corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 1.00 ea | SN9133N | Allgood Hardware 280x46x33mm Concealed Overhead Door closer, with finished track & arm for Single Action Doors, adjustable power 2-4, closing force, latch action & cushion stop, Certifire approved CF6022 for use on up to 60 minute timber fire doors & CE Marked to BS EN1154: 3-8-4/2-1-1-3, 10 year manufacturer warranty, SNP finish |
| 1.00 ea | ZQ0067743 \* | SS9133NMHO Allgood Hardware 280x46x33mm Concealed Overhead Door closer, with finished track & arm c/w Mechanical Hold Open device \*Not for use on Fire doors\*, for Single Action Doors, adjustable power 2-4, closing force, latch action & cushion stop, CE Marked to BS EN1154: 3-8-4/2-1-1-3, 10 year manufacturer warranty, SNP finish |
| 1.00 pr | SS1763NBB \* | Allgood Mode® 1300x67x19mm entrance pull handle with back to back fixings at 1200mm centres for doors 35-54mm thickness with glass fixings sold separately, grade 316, satin stainless finish |
| 2.00 ea | SS48800F | Allgood Hardware 203x19x11mm Lever Action Flush bolt, with coil spring, parallel movement radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48800FP] |
| 1.00 ea | SS7051 | Allgood Hardware 63x20x38mm easi-clean socket for wood or stone, grade 316, satin stainless finish |
| 1.00 ea | ZQ0062637 \* | Allgood Hardware 900x450x1.5mm Satin Stainless Steel Kick Plate. Undrilled.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | ZQ0062638 \* | Allgood Hardware 400x450x1.5mm Satin Stainless Steel Kick Plate. Undrilled.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | XX90010 \* | See Remarks |
| 1.00 ea | SS2301 | Allgood Hardware 38x47mm Heavy Duty Circular Floor Mounted Door Stop, grade 316, 25 year manufacturing warranty, satin stainless steel finish |

|  |
| --- |
| Total GBP: 734.20 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.01.16.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| Assumme Doors to have plain meeting stiles. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 0110 -** | **FOH - Leaf & half access controlled circulation door - DRT-04a - FWD/15/05/c/FD60/AC- nds - BLA** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 6.00 ea | SS8066R | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with radius corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 1.00 ea | XX10508FPN | Allgood Hardware intumescent pack for 10508 jamb mounted closer, suitable for timber doors in FD30/60 applications |
| 1.00 ea | XX9134FPN \* | Allgood Hardware Size 3-6 Concealed Cam Closer Intumescent Pack to suit 9134N |
| 1.00 ea | SC10508 | Allgood Hardware fully concealed jamb fixed door closer, CE Marked to BS EN: 1154 classification 3-8-3-1-1-3, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 240 minutes on metal doors, satin chrome plated finish (For Fire Pack not supplied order XX10508FPN) |
| 1.00 ea | SN9134N | Allgood Hardware 293x54x40mm Concealed Overhead Door closer, with finished track & arm for Single Action Doors, adjustable power 3-6, closing force, latch action & cushion stop, Certifire approved CF6022 for use on up to 60 minute timber fire doors & CE Marked to BS EN1154: 3-8-6/3-1-1-3, 10 year manufacturer warranty, SNP finish |
| 12.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 2.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | SS1761 | Allgood Mode® 700x67x19mm entrance pull handle with bolt through fixings at 600mm centres, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 4.00 ea | SS8449 | Allgood Hardware 76mm circular 'Fire door keep shut' symbol, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, satin stainless steel finish |
| 1.00 ea | XX75574D \* | Allgood Secure 520x52x28mm Surface Mounted Architectural Electromagnet and Armature, for use on double door applications, 300kg holding force (on each door leaf), MBS monitored and dual 12/24 DC voltage, with 500ma current draw @ 12 volts and 250ma current draw @ 24 volts, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 60 minutes on metal doors |
| 1.00 ea | XX90009 \* | Access control to be supplied by others |

|  |
| --- |
| Total GBP: 1,467.60 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.00.ST10.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| Access Control By Others. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 0111 -** | **BOH - Single access controlled circulation door - DRT-02 - BWD/01/05/a/FD60/AC - nds** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 4.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 8.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |
| 1.00 ea | XX75574 | Allgood Secure 270x52x28mm surface mounted architectural electromagnet and armature for use on single door applications, 300kg holding force, MBS monitored and dual 12/24 DC voltage with 250ma current draw @ 12 volts and 125ma current draw @ 24 volts, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 60 minutes on metal doors |
| 1.00 ea | XX75574ZLC \* | Allgood Secure Z and L bracket armature assembly complete with architectural cover for use with XX75574 electromagnet. For use on inward opening doors only. |
| 1.00 ea | XX90009 \* | Access control to be supplied by others |

|  |
| --- |
| Total GBP: 655.42 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.PL23.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 0112 -** | **BOH - Double circulation door - DRT-01 - BWD/02/05/a/FD60/Fig6 - 1 ds** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 8.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 16.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S66 | Allgood Hardware, Figure 6, soffit bracket & template, satin stainless steel finish |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 2.00 ea | XX97948SS | Allgood Alite® FDKLS 76øx1.2mm 'Fire Door Keep Locked Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | SS48800F | Allgood Hardware 203x19x11mm Lever Action Flush bolt, with coil spring, parallel movement radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48800FP] |
| 1.00 ea | SS48801F | Allgood Hardware 457x19mm Lever Action Flush bolt, with coil spring, parallel movement, radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48801FP] |
| 1.00 ea | SS7051 | Allgood Hardware 63x20x38mm easi-clean socket for wood or stone, grade 316, satin stainless finish |
| 1.00 ea | XX48800FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48800 flush bolts |
| 1.00 ea | XX48801FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48801 flush bolts |
| 2.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |

|  |
| --- |
| Total GBP: 754.82 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.00.045A.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| We have assumed doors have plain meeting stiles.  Are both leaves required to be active? |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 0113 -** | **BOH - Double circulation door - DRT-01 - BWD/02/05/a/FD60/Fig1 - 1 ds** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 1.00 ea | SS7636F \* | Spare Radius Strike Plate for Deadlock New 76 Series SS7686FS60 |
| 8.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 16.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | SN7319BM \* | Allgood Hardware 'B' 70mm (35/35) length Euro Profile Cylinder & turn, independently tested to BS EN 1303:2015 classification 1/6/0/B\*1/0/C/6/D, trademark protection 6 pin cylinder with solid and lateral profile pins, c/w “anti-Bump”, “anti-pick”, “anti-drill” and “anti-pull” protection, 2 keyed, under master key, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors, satin nickel plated finish |
| 1.00 ea | SS7686FN60 | Allgood Hardware 93x60mm backset profile cylinder mortice deadlock case only, double throw 20mm deadbolt, CE Marked to BS EN 12209 3/X/8/1/0/G/2/B/C/0/0, Certifire approved CF5899 for use up to 120 minutes on timber fire doors and 240 minute metal fire doors, radius forend & square strike, satin stainless steel finish |
| 1.00 ea | XX7679FP1 | Allgood Hardware intumescent Pack for 76 Series 60mm Backset TFD30, TFD60 |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 2.00 ea | XX97876SS | Allgood Alite® Cylinder Rose, 50mm diameter concealed with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 60 minute timber doors, satin stainless steel finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 2.00 ea | XX97948SS | Allgood Alite® FDKLS 76øx1.2mm 'Fire Door Keep Locked Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | SS48800F | Allgood Hardware 203x19x11mm Lever Action Flush bolt, with coil spring, parallel movement radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48800FP] |
| 1.00 ea | SS48801F | Allgood Hardware 457x19mm Lever Action Flush bolt, with coil spring, parallel movement, radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48801FP] |
| 1.00 ea | SS7051 | Allgood Hardware 63x20x38mm easi-clean socket for wood or stone, grade 316, satin stainless finish |
| 1.00 ea | XX48800FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48800 flush bolts |
| 1.00 ea | XX48801FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48801 flush bolts |
| 2.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |

|  |
| --- |
| Total GBP: 840.38 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.00.045A.02 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| We have assumed doors have plain meeting stiles.  Are both leaves required to be active? |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 0114 -** | **FOH - Single lockable door (FD30) 2.2 - nds - DRT-34** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 3.00 ea | SS8066R | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with radius corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 3.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SN7319AM \* | Allgood Hardware 'A' 60mm (30/30) length Euro Profile Cylinder & turn, independently tested to BS EN 1303:2015 classification 1/6/0/B\*1/0/C/6/D, trademark protection 6 pin cylinder with solid and lateral profile pins, c/w “anti-Bump”, “anti-pick”, “anti-drill” and “anti-pull” protection, 2 keyed, under master key, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors, satin nickel finish |
| 1.00 ea | SS7286F60 | Allgood Hardware 92x60mm backset HL series profile cylinder mortice deadlock case only, single throw 20mm Stainless Steel deadbolt, rounded forend & strike CE Marked to BS EN: 12209 3/X/8/1/0/G/2/B/A/0/0 Certifire approved CF347 for use on 90 minute timber fire doors and up to 240 minutes for metal fire doors, 10 year manufacturing warranty, satin stainless steel finish |
| 1.00 ea | XX7286FP6 | Allgood Hardware intumescent Lock Fire Pack 7286 60mm backset Series |
| 2.00 ea | SS796Q | Allgood Modric® 50x4mm Circular Escutcheon for Euro Profile Cylinder, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and for up to 240 minutes on metal doors, grade 316, 25 year manufacturing warranty, satin stainless steel finish |
| 1.00 pr | SS1761BB | Allgood Mode® 700x67x19mm entrance pulls, back to back fixings at 600mm centres for doors 35-54mm thickness with glass fixings sold separately, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | SS2301 | Allgood Hardware 38x47mm Heavy Duty Circular Floor Mounted Door Stop, grade 316, 25 year manufacturing warranty, satin stainless steel finish |
| 2.00 ea | SS8449 | Allgood Hardware 76mm circular 'Fire door keep shut' symbol, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, satin stainless steel finish |

|  |
| --- |
| Total GBP: 429.01 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.01.08.02 | PM.DR.01.08.03 |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 0115 -** | **BOH - Double lockable door w/levers 2.2 (FD) - DRT-45 - FD120** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 1.00 ea | XX48810B \* | Allgood Hardware Barza Bolt Keep type B – top mounting door opening outward |
| 1.00 ea | XX48810E \* | Barza Bolt Easy Clean Socket Type E |
| 8.00 ea | SS8064 | Allgood Hardware 100x100x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with square corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to BS EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 16.00 ea | XX8064FP | Allgood Hardware 98x39x1mm intumescent pack to suit 8064 & 97502 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | XX98141S66 | Allgood Hardware, Figure 6, soffit bracket & template, satin stainless steel finish |
| 1.00 ea | SS7679FN60 | Allgood Hardware 93x60mm backset profile cylinder mortice lock case only, heavy sprung for levers, double throw deadbolt, CE Marked to BS EN 12209 3/X/8/1/0/G/2/B/C/2/0, Certifire approved CF5899 for use up to 120 minutes on timber fire doors and 240 minute metal fire doors, radius forend & square strike, satin stainless steel finish |
| 1.00 ea | XX7679FP2 \* | Allgood Hardware intumescent Pack for 76 Series 60mm Backset TFD90 and TFD120 |
| 1.00 pr | XX97422SSN | Allgood Alite® 134 x 64mm x 19mmØ Safety lever handles, on Quadaxial® 50Ø x 4mm concealed fixing roses (tested to 1 million cycles), meets BS 8300 and “Doc M”, independently tested to BS EN 1906 4/7/-/1/0/3/0/U, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, suitable for doors 35-54mm, grade 304, satin stainless steel finish |
| 1.00 ea | XX9066T | Allgood Hardware 8mm HT Spindle, suitable for 45-64mm doors |
| 2.00 ea | MT04100BZ \* | Allgood Hardware M4 x 100mm Long Pozi countersunk screws, to suit door thicknesses 56-90mm, A2 stainless steel |
| 1.00 ea | SN7319CM \* | Allgood Hardware 'C' 80mm (40/40) length Euro Profile Cylinder & turn, independently tested to BS EN 1303:2015 classification 1/6/0/B\*1/0/C/6/D, trademark protection 6 pin cylinder with solid and lateral profile pins, c/w “anti-Bump”, “anti-pick”, “anti-drill” and “anti-pull” protection, 2 keyed, under master key, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors, satin nickel finish |
| 2.00 ea | XX97876SS | Allgood Alite® Cylinder Rose, 50mm diameter concealed with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 60 minute timber doors, satin stainless steel finish |
| 2.00 ea | XX97948SS | Allgood Alite® FDKLS 76øx1.2mm 'Fire Door Keep Locked Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 2.00 ea | SS48810 \* | Allgood Hardware Barza Bolt 220mm, high security for internal or external doors, tamper and abuse resistant, suitable for use on FD30 fire doors, fully concealed fixings, grade 304, stainless steel finish |
| 2.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |

|  |
| --- |
| Total GBP: 1,101.12 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.PL02.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| FD120 fire rating noted.  Not all items of hardware specified have been tested to FD120 ( cylinders , lever handles , escutcheons )  Please confirm this with your FD120 fire door manufacturers primary fire test evidence. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 0116 -** | **FOH - Single lockable circulation door - DRT-02a - FWD/01/06/c/FD60 - KP** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 4.00 ea | SS8066R | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with radius corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 1.00 ea | SN9133N | Allgood Hardware 280x46x33mm Concealed Overhead Door closer, with finished track & arm for Single Action Doors, adjustable power 2-4, closing force, latch action & cushion stop, Certifire approved CF6022 for use on up to 60 minute timber fire doors & CE Marked to BS EN1154: 3-8-4/2-1-1-3, 10 year manufacturer warranty, SNP finish |
| 8.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX9133FPN \* | Allgood Hardware Size 2-4 Concealed Cam Closer Intumescent Pack for use on up to 60 minute timber fire doors to suit 9133N |
| 1.00 ea | SN7319BM \* | Allgood Hardware 'B' 70mm (35/35) length Euro Profile Cylinder & turn, independently tested to BS EN 1303:2015 classification 1/6/0/B\*1/0/C/6/D, trademark protection 6 pin cylinder with solid and lateral profile pins, c/w “anti-Bump”, “anti-pick”, “anti-drill” and “anti-pull” protection, 2 keyed, under master key, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors, satin nickel plated finish |
| 1.00 ea | SS7286F60 | Allgood Hardware 92x60mm backset HL series profile cylinder mortice deadlock case only, single throw 20mm Stainless Steel deadbolt, rounded forend & strike CE Marked to BS EN: 12209 3/X/8/1/0/G/2/B/A/0/0 Certifire approved CF347 for use on 90 minute timber fire doors and up to 240 minutes for metal fire doors, 10 year manufacturing warranty, satin stainless steel finish |
| 1.00 ea | XX7286FP6 | Allgood Hardware intumescent Lock Fire Pack 7286 60mm backset Series |
| 1.00 ea | SS1761 | Allgood Mode® 700x67x19mm entrance pull handle with bolt through fixings at 600mm centres, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | SS796Q | Allgood Modric® 50x4mm Circular Escutcheon for Euro Profile Cylinder, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and for up to 240 minutes on metal doors, grade 316, 25 year manufacturing warranty, satin stainless steel finish |
| 2.00 ea | SS8449 | Allgood Hardware 76mm circular 'Fire door keep shut' symbol, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, satin stainless steel finish |
| 1.00 ea | SS2301 | Allgood Hardware 38x47mm Heavy Duty Circular Floor Mounted Door Stop, grade 316, 25 year manufacturing warranty, satin stainless steel finish |
| 1.00 ea | ZQ0062637 \* | Allgood Hardware 900x450x1.5mm Satin Stainless Steel Kick Plate. Undrilled.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |

|  |
| --- |
| Total GBP: 563.76 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.00.58.04 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 0117 -** | **FOH - Single access controlled circulation door - DRT-34 - FWD/01/05/c/FD30/AC** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 3.00 ea | SS8066R | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with radius corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 3.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SS1761 | Allgood Mode® 700x67x19mm entrance pull handle with bolt through fixings at 600mm centres, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | XX75574 | Allgood Secure 270x52x28mm surface mounted architectural electromagnet and armature for use on single door applications, 300kg holding force, MBS monitored and dual 12/24 DC voltage with 250ma current draw @ 12 volts and 125ma current draw @ 24 volts, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 60 minutes on metal doors |
| 1.00 ea | XX75574ZLC \* | Allgood Secure Z and L bracket armature assembly complete with architectural cover for use with XX75574 electromagnet. For use on inward opening doors only. |
| 2.00 ea | SS8449 | Allgood Hardware 76mm circular 'Fire door keep shut' symbol, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, satin stainless steel finish |
| 1.00 ea | SS2301 | Allgood Hardware 38x47mm Heavy Duty Circular Floor Mounted Door Stop, grade 316, 25 year manufacturing warranty, satin stainless steel finish |
| 1.00 ea | XX90009 \* | Access control to be supplied by others |

|  |
| --- |
| Total GBP: 488.91 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.01.42.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 0118 -** | **BOH - Single staff accessible WC door - DRT-02a - BWD/01/08/D/ST/FD30 - Outward Opening** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 3.00 ea | SS8066 | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with square corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to BS EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 3.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | XX98141S66 | Allgood Hardware, Figure 6, soffit bracket & template, satin stainless steel finish |
| 1.00 ea | SS7608FN60 | Allgood Hardware 93x60mm backset bathroom lock case only, heavy sprung for levers, CE Marked to BS EN 12209 3/X/8/1/0/G/-/B/0/2/0, Certifire approved CF5899 for use up to 120 minutes on timber fire doors and 240 minute metal fire doors, with radius forend & square strike satin stainless steel finish |
| 1.00 ea | XX7679FP1 | Allgood Hardware intumescent Pack for 76 Series 60mm Backset TFD30, TFD60 |
| 1.00 pr | XX97422SSN | Allgood Alite® 134 x 64mm x 19mmØ Safety lever handles, on Quadaxial® 50Ø x 4mm concealed fixing roses (tested to 1 million cycles), meets BS 8300 and “Doc M”, independently tested to BS EN 1906 4/7/-/1/0/3/0/U, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, suitable for doors 35-54mm, grade 304, satin stainless steel finish |
| 1.00 ea | XX97874SS | Allgood Alite® W/C turn, easy operation large turn & indicator release set, on 50mm diameter concealed fixing rose, with 8mm spindle & back to back fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 60 minute timber doors, satin stainless steel finish |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 1.00 ea | XX97935SS | Allgood Alite® 76øx1.2mm 'Disabled' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | SS16051N | Allgood Modric® 32øx632x95mm Support Grab Rail, with concealed fixings at 600mm centres, complete with 50mmøx3mm thrust roses, In accordance with the recommendations of BS 8300 and Approved Document M, grade 316, satin stainless steel finish |
| 2.00 ea | XX98230SS | Allgood Alite® Hat & Coat Hook, satin stainless steel finish |

|  |
| --- |
| Total GBP: 367.77 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.25.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| Door schedule requests lever handles ( LH/LH ) however the notes request 1M high push plate?  Please confirm. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 0119 -** | **BOH - Single staff accessible WC/Shower door - DRT-02a - BWD/01/08/D/ST/S/FD30 - Inward Opening** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 1.00 ea | SS9135D | Geze Boxer 288x45x32mm concealed overhead door closer with finished track, arm, top centre & pivot for double action doors adjustable power 2-4, closing force, latch action & backcheck Certifire approved & CE marked to BS EN 1154: 3-8-4/3-1-1-4, for use on timber fire doors up to 60 minutes and metal fire doors up to 240 minutes, stainless steel finish, (order separate intumescent kit XX9135FP) |
| 1.00 ea | XX9135FP | intumescent pack for use with 9135D Geze Boxer concealed door closers use 1 for FD30 and 2 for FD60 |
| 1.00 ea | SS7608FN60 | Allgood Hardware 93x60mm backset bathroom lock case only, heavy sprung for levers, CE Marked to BS EN 12209 3/X/8/1/0/G/-/B/0/2/0, Certifire approved CF5899 for use up to 120 minutes on timber fire doors and 240 minute metal fire doors, with radius forend & square strike satin stainless steel finish |
| 1.00 ea | XX7679FP1 | Allgood Hardware intumescent Pack for 76 Series 60mm Backset TFD30, TFD60 |
| 1.00 pr | XX97422SSN | Allgood Alite® 134 x 64mm x 19mmØ Safety lever handles, on Quadaxial® 50Ø x 4mm concealed fixing roses (tested to 1 million cycles), meets BS 8300 and “Doc M”, independently tested to BS EN 1906 4/7/-/1/0/3/0/U, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, suitable for doors 35-54mm, grade 304, satin stainless steel finish |
| 1.00 ea | XX97874SS | Allgood Alite® W/C turn, easy operation large turn & indicator release set, on 50mm diameter concealed fixing rose, with 8mm spindle & back to back fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 60 minute timber doors, satin stainless steel finish |
| 1.00 ea | XX13006 | Allgood Hardware Emergency Release Door Stop 80x40x45mm, with hold back facility |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 1.00 ea | XX97935SS | Allgood Alite® 76øx1.2mm 'Disabled' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | XX97956SS | Allgood Alite® 76øx1.2mm 'Shower' Symbol disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | SS16051N | Allgood Modric® 32øx632x95mm Support Grab Rail, with concealed fixings at 600mm centres, complete with 50mmøx3mm thrust roses, In accordance with the recommendations of BS 8300 and Approved Document M, grade 316, satin stainless steel finish |
| 2.00 ea | XX98230SS | Allgood Alite® Hat & Coat Hook, satin stainless steel finish |

|  |
| --- |
| Total GBP: 679.72 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.24.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| Door schedule requests lever handles ( LH/LH ) however the notes request 1M high push plate?  Please confirm. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 0120 -** | **FOH - Single Gender Neutral WC door - 1m pulls - Without Door Stop - DRT-34 - FWD/01/08/GN** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 3.00 ea | SS8066 | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with square corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to BS EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 1.00 ea | SS7518N | Allgood Hardware 76x58mm backset cubicle mortice deadlock with 8mm follower, satin stainless steel finish |
| 1.00 ea | SS1763 \* | Allgood Mode® 1000x67x19mm entrance pull handle with bolt through fixings at 900mm centres, grade 316, satin stainless steel finish |
| 1.00 ea | SS771Q2529 | Allgood Modric® 37x17x18mm WC Turn on 50mmø x 4mm rose, complete with emergency release rose with indicator and 5-8mm spindle, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 60 minute timber doors, 25 year manufacturing warranty, satin stainless steel finish. |
| 1.00 ea | SS8433 | Allgood Modric® 76mm circular Female symbol, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, satin stainless steel finish |
| 1.00 ea | ZQ0069803 \* | Allgood Hardware 1000x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixing -  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | SS6542 | Allgood Modric® 14mmø x 75mm buffer coat hook with pin and concealed fixing, grade 316, satin stainless steel finish |
| 1.00 ea | XX90010 \* | See Remarks |

|  |
| --- |
| Total GBP: 263.51 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.28.03A |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| Ironmongery schedule requests lever handles ( LH/LH ) and 1 m high push plate?  Please confirm. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 0121 -** | **BOH - Single accessible WC door - Outward Opening DRT-02 - BWD/01/08/D - No Door Stop** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 4.00 ea | SS97501 | Allgood Hardware 102x76x3mm Butt Hinges, with square corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 1.00 ea | SS7608FN60 | Allgood Hardware 93x60mm backset bathroom lock case only, heavy sprung for levers, CE Marked to BS EN 12209 3/X/8/1/0/G/-/B/0/2/0, Certifire approved CF5899 for use up to 120 minutes on timber fire doors and 240 minute metal fire doors, with radius forend & square strike satin stainless steel finish |
| 1.00 pr | XX97422SSN | Allgood Alite® 134 x 64mm x 19mmØ Safety lever handles, on Quadaxial® 50Ø x 4mm concealed fixing roses (tested to 1 million cycles), meets BS 8300 and “Doc M”, independently tested to BS EN 1906 4/7/-/1/0/3/0/U, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, suitable for doors 35-54mm, grade 304, satin stainless steel finish |
| 1.00 ea | XX97873SS | Allgood Alite® 'easy operation' Turn & Indicator Release Set, on covered 50mm diameter roses with 8mm spindle & back to back fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 60 minute timber doors, satin stainless steel finish |
| 1.00 ea | XX97935SS | Allgood Alite® 76øx1.2mm 'Disabled' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | SS16051N | Allgood Modric® 32øx632x95mm Support Grab Rail, with concealed fixings at 600mm centres, complete with 50mmøx3mm thrust roses, In accordance with the recommendations of BS 8300 and Approved Document M, grade 316, satin stainless steel finish |
| 2.00 ea | XX98230SS | Allgood Alite® Hat & Coat Hook, satin stainless steel finish |
| 2.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |

|  |
| --- |
| Total GBP: 670.88 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.BM.06.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 0122 -** | **BOH - Single WC door - DRT-02a - BWD/01/08** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 4.00 ea | SS97501 | Allgood Hardware 102x76x3mm Butt Hinges, with square corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 1.00 ea | SS7608FN60 | Allgood Hardware 93x60mm backset bathroom lock case only, heavy sprung for levers, CE Marked to BS EN 12209 3/X/8/1/0/G/-/B/0/2/0, Certifire approved CF5899 for use up to 120 minutes on timber fire doors and 240 minute metal fire doors, with radius forend & square strike satin stainless steel finish |
| 1.00 pr | XX97423SSN | Allgood Alite® 127 x 64mm x 19mmØ Straight lever handles, on Quadaxial® 50Ø x 4mm concealed fixing roses (tested to 1 million cycles), independently tested to BS EN 1906 4/7/-/1/0/3/0/U, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, suitable for doors 35-54mm, grade 304, satin stainless steel finish |
| 1.00 ea | XX97873SS | Allgood Alite® 'easy operation' Turn & Indicator Release Set, on covered 50mm diameter roses with 8mm spindle & back to back fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 60 minute timber doors, satin stainless steel finish |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 1.00 ea | XX98230SS | Allgood Alite® Hat & Coat Hook, satin stainless steel finish |

|  |
| --- |
| Total GBP: 125.53 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.00.31.01 | PM.DR.00.41.02 |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 0123 -** | **BOH - Single accessible WC door - DRT-43A - BWD/01/08/D - Inward Opening** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 1.00 ea | ZQ0062468 \* | Allgood Hardware Satin Stainless Steel Heavy Duty Floor Pivot 200kg Max door weight. Supplied with 20mm Extended Spindle. |
| 1.00 ea | SS9231DTC | Allgood Hardware Double Action Top Centre & Cover Plate, satin stainless steel finish |
| 1.00 ea | ZQ0062469 \* | Bottom Strap to suit pivot floor pivot ZQ0062468 |
| 1.00 ea | SS7608FN60 | Allgood Hardware 93x60mm backset bathroom lock case only, heavy sprung for levers, CE Marked to BS EN 12209 3/X/8/1/0/G/-/B/0/2/0, Certifire approved CF5899 for use up to 120 minutes on timber fire doors and 240 minute metal fire doors, with radius forend & square strike satin stainless steel finish |
| 1.00 pr | XX97422SSN | Allgood Alite® 134 x 64mm x 19mmØ Safety lever handles, on Quadaxial® 50Ø x 4mm concealed fixing roses (tested to 1 million cycles), meets BS 8300 and “Doc M”, independently tested to BS EN 1906 4/7/-/1/0/3/0/U, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, suitable for doors 35-54mm, grade 304, satin stainless steel finish |
| 1.00 ea | XX97874SS | Allgood Alite® W/C turn, easy operation large turn & indicator release set, on 50mm diameter concealed fixing rose, with 8mm spindle & back to back fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 60 minute timber doors, satin stainless steel finish |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 1.00 ea | XX13006 | Allgood Hardware Emergency Release Door Stop 80x40x45mm, with hold back facility |
| 1.00 ea | XX97935SS | Allgood Alite® 76øx1.2mm 'Disabled' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | SS16051N | Allgood Modric® 32øx632x95mm Support Grab Rail, with concealed fixings at 600mm centres, complete with 50mmøx3mm thrust roses, In accordance with the recommendations of BS 8300 and Approved Document M, grade 316, satin stainless steel finish |
| 2.00 ea | XX98230SS | Allgood Alite® Hat & Coat Hook, satin stainless steel finish |

|  |
| --- |
| Total GBP: 529.35 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.00.32.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 0124 -** | **FOH - Single School Arrivals ACC WC - Inward Opening - PH - DRT-43A** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 1.00 ea | ZQ0062468 \* | Allgood Hardware Satin Stainless Steel Heavy Duty Floor Pivot 200kg Max door weight. Supplied with 20mm Extended Spindle. |
| 1.00 ea | XX13006 | Allgood Hardware Emergency Release Door Stop 80x40x45mm, with hold back facility |
| 1.00 ea | ZQ0062469 \* | Bottom Strap to suit pivot floor pivot ZQ0062468 |
| 1.00 ea | SS7518FN | Allgood Hardware 76x58mm cubicle mortice deadlock, 8mm follower, radiused, satin stainless steel finish |
| 1.00 ea | SS9231DTC | Allgood Hardware Double Action Top Centre & Cover Plate, satin stainless steel finish |
| 1.00 ea | SS771Q2530 | Allgood Modric® 50mm dia x 4mm rose and disabled WC turn for bathroom locks, complete with external release/indicator, 5-8mm spindle, 38mm centres with 90 degrees turn action, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 60 minute timber doors, grade 316, 25 year manufacturing warranty, satin stainless steel finish |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | SS8435 | Allgood Modric® 76mm circular wheelchair accessible toilet symbol, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, satin stainless finish |
| 1.00 ea | SS16051N | Allgood Modric® 32øx632x95mm Support Grab Rail, with concealed fixings at 600mm centres, complete with 50mmøx3mm thrust roses, In accordance with the recommendations of BS 8300 and Approved Document M, grade 316, satin stainless steel finish |
| 2.00 ea | SS6542 | Allgood Modric® 14mmø x 75mm buffer coat hook with pin and concealed fixing, grade 316, satin stainless steel finish |

|  |
| --- |
| Total GBP: 632.36 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.00.07b.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 0125 -** | **FOH - Single School Arrivals WC door - Outward Opening - PH - DRT-02a** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 4.00 ea | SS8066 | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with square corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to BS EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 1.00 ea | SS7518FN | Allgood Hardware 76x58mm cubicle mortice deadlock, 8mm follower, radiused, satin stainless steel finish |
| 1.00 ea | SS771Q2529 | Allgood Modric® 37x17x18mm WC Turn on 50mmø x 4mm rose, complete with emergency release rose with indicator and 5-8mm spindle, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 60 minute timber doors, 25 year manufacturing warranty, satin stainless steel finish. |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | SS8434 | Allgood Modric® 76mm circular Unisex symbol, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, satin stainless steel finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | SS6541 | Allgood Modric® 14mmø x 38mm coat hook with pin and concealed fixing, grade 316, 25 year manufacturer warranty,satin stainless steel finish |

|  |
| --- |
| Total GBP: 257.84 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.00.54.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 0126 -** | **FOH - Single male WC entrance door - DRT-02a - FWD/01/05/c/M** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 4.00 ea | SS8066 | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with square corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to BS EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 1.00 ea | SN9133N | Allgood Hardware 280x46x33mm Concealed Overhead Door closer, with finished track & arm for Single Action Doors, adjustable power 2-4, closing force, latch action & cushion stop, Certifire approved CF6022 for use on up to 60 minute timber fire doors & CE Marked to BS EN1154: 3-8-4/2-1-1-3, 10 year manufacturer warranty, SNP finish |
| 1.00 ea | SS1761 | Allgood Mode® 700x67x19mm entrance pull handle with bolt through fixings at 600mm centres, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | SS8432 | Allgood Modric® 76mmx2mm circular Male symbol, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, satin stainless steel finish |
| 1.00 ea | SS2301 | Allgood Hardware 38x47mm Heavy Duty Circular Floor Mounted Door Stop, grade 316, 25 year manufacturing warranty, satin stainless steel finish |

|  |
| --- |
| Total GBP: 332.40 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.00.14.05 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 0127 -** | **FOH - Single female WC entrance door - DRT-02a - FWD/01/05/c/F** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 4.00 ea | SS8066 | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with square corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to BS EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 1.00 ea | SN9133N | Allgood Hardware 280x46x33mm Concealed Overhead Door closer, with finished track & arm for Single Action Doors, adjustable power 2-4, closing force, latch action & cushion stop, Certifire approved CF6022 for use on up to 60 minute timber fire doors & CE Marked to BS EN1154: 3-8-4/2-1-1-3, 10 year manufacturer warranty, SNP finish |
| 1.00 ea | SS1761 | Allgood Mode® 700x67x19mm entrance pull handle with bolt through fixings at 600mm centres, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | SS8433 | Allgood Modric® 76mm circular Female symbol, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, satin stainless steel finish |
| 1.00 ea | SS2301 | Allgood Hardware 38x47mm Heavy Duty Circular Floor Mounted Door Stop, grade 316, 25 year manufacturing warranty, satin stainless steel finish |

|  |
| --- |
| Total GBP: 332.40 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.00.13.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 0128 -** | **FOH - Single staff WC entrance door - DRT-34 - FWD/01/05/a/ST/FD60** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 4.00 ea | SS8066 | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with square corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to BS EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 8.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SS1761 | Allgood Mode® 700x67x19mm entrance pull handle with bolt through fixings at 600mm centres, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 2.00 ea | SS8449 | Allgood Hardware 76mm circular 'Fire door keep shut' symbol, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, satin stainless steel finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | SS2301 | Allgood Hardware 38x47mm Heavy Duty Circular Floor Mounted Door Stop, grade 316, 25 year manufacturing warranty, satin stainless steel finish |
| 1.00 ea | SS8451 \* | Allgood Modric® 76ømmx2.5mm 'WC' signage with torx screw fixings, satin stainless steel finish |
| 1.00 ea | SS8454 \* | Allgood Modric® 76ømmx2.5mm 'Staff' signage with torx screw fixings, satin stainless steel finish |

|  |
| --- |
| Total GBP: 300.25 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.01.06.06 | PM.DR.01.59.01 |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 0129 -** | **FOH - Single accessible WC door - DRT-34 - FWD/01/08/D - Outward Opening** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 3.00 ea | SS8066 | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with square corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to BS EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 1.00 ea | SS7208F60 | Allgood Hardware 92x60mm backset HL Series Bathroom Lock case only, with stainless steel low friction latchbolt, unique griptight follower, heavy sprung for levers, rounded forend & strike, Certifire approved CF347 for use on 90 minute timber fire doors and up to 240 minutes for metal fire doors, 10 year manufacturing warranty, satin stainless steel finish |
| 1.00 pr | XX97422SSN | Allgood Alite® 134 x 64mm x 19mmØ Safety lever handles, on Quadaxial® 50Ø x 4mm concealed fixing roses (tested to 1 million cycles), meets BS 8300 and “Doc M”, independently tested to BS EN 1906 4/7/-/1/0/3/0/U, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, suitable for doors 35-54mm, grade 304, satin stainless steel finish |
| 1.00 ea | SS771Q2530 | Allgood Modric® 50mm dia x 4mm rose and disabled WC turn for bathroom locks, complete with external release/indicator, 5-8mm spindle, 38mm centres with 90 degrees turn action, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 60 minute timber doors, grade 316, 25 year manufacturing warranty, satin stainless steel finish |
| 1.00 ea | SS8435 | Allgood Modric® 76mm circular wheelchair accessible toilet symbol, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, satin stainless finish |
| 1.00 ea | SS16051N | Allgood Modric® 32øx632x95mm Support Grab Rail, with concealed fixings at 600mm centres, complete with 50mmøx3mm thrust roses, In accordance with the recommendations of BS 8300 and Approved Document M, grade 316, satin stainless steel finish |
| 2.00 ea | SS6541 | Allgood Modric® 14mmø x 38mm coat hook with pin and concealed fixing, grade 316, 25 year manufacturer warranty,satin stainless steel finish |

|  |
| --- |
| Total GBP: 319.81 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.01.24.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| Would advise self closing to contain bad odurs from the wc's. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 0130 -** | **FOH - Single Staff WC door - With Door Stop - DRT-34 - FWD/01/08/S** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 3.00 ea | SS8066 | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with square corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to BS EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 1.00 ea | SS7518N | Allgood Hardware 76x58mm backset cubicle mortice deadlock with 8mm follower, satin stainless steel finish |
| 1.00 ea | SS1763 \* | Allgood Mode® 1000x67x19mm entrance pull handle with bolt through fixings at 900mm centres, grade 316, satin stainless steel finish |
| 1.00 ea | SS771Q2529 | Allgood Modric® 37x17x18mm WC Turn on 50mmø x 4mm rose, complete with emergency release rose with indicator and 5-8mm spindle, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 60 minute timber doors, 25 year manufacturing warranty, satin stainless steel finish. |
| 1.00 ea | ZQ0069803 \* | Allgood Hardware 1000x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixing -  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 1.00 ea | SS8451 \* | Allgood Modric® 76ømmx2.5mm 'WC' signage with torx screw fixings, satin stainless steel finish |
| 1.00 ea | SS8454 \* | Allgood Modric® 76ømmx2.5mm 'Staff' signage with torx screw fixings, satin stainless steel finish |
| 1.00 ea | SS6541 | Allgood Modric® 14mmø x 38mm coat hook with pin and concealed fixing, grade 316, 25 year manufacturer warranty,satin stainless steel finish |
| 1.00 ea | XX90010 \* | See Remarks |

|  |
| --- |
| Total GBP: 270.48 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.01.25.01 | PM.DR.01.26.01 |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| Would advise self closing to contain bad odurs from the wc's. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 0131 -** | **FOH - Accessible WC - Inward Opening - PH - DRT-43A** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 1.00 ea | ZQ0062468 \* | Allgood Hardware Satin Stainless Steel Heavy Duty Floor Pivot 200kg Max door weight. Supplied with 20mm Extended Spindle. |
| 1.00 ea | XX13006 | Allgood Hardware Emergency Release Door Stop 80x40x45mm, with hold back facility |
| 1.00 ea | ZQ0062469 \* | Bottom Strap to suit pivot floor pivot ZQ0062468 |
| 1.00 ea | SS7518FN | Allgood Hardware 76x58mm cubicle mortice deadlock, 8mm follower, radiused, satin stainless steel finish |
| 1.00 ea | SS9231DTC | Allgood Hardware Double Action Top Centre & Cover Plate, satin stainless steel finish |
| 1.00 ea | SS771Q2530 | Allgood Modric® 50mm dia x 4mm rose and disabled WC turn for bathroom locks, complete with external release/indicator, 5-8mm spindle, 38mm centres with 90 degrees turn action, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 60 minute timber doors, grade 316, 25 year manufacturing warranty, satin stainless steel finish |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | SS2301 | Allgood Hardware 38x47mm Heavy Duty Circular Floor Mounted Door Stop, grade 316, 25 year manufacturing warranty, satin stainless steel finish |
| 1.00 ea | SS8435 | Allgood Modric® 76mm circular wheelchair accessible toilet symbol, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, satin stainless finish |
| 1.00 ea | SS16051N | Allgood Modric® 32øx632x95mm Support Grab Rail, with concealed fixings at 600mm centres, complete with 50mmøx3mm thrust roses, In accordance with the recommendations of BS 8300 and Approved Document M, grade 316, satin stainless steel finish |
| 2.00 ea | SS6541 | Allgood Modric® 14mmø x 38mm coat hook with pin and concealed fixing, grade 316, 25 year manufacturer warranty,satin stainless steel finish |

|  |
| --- |
| Total GBP: 627.53 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.01.18b.01 | PM.DR.01.33.01 |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 02 -** | **BOH - Double - DRT-01 - BWD/02/05/a/FD30/AC** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 8.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 8.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | XX97948SS | Allgood Alite® FDKLS 76øx1.2mm 'Fire Door Keep Locked Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | SS48800F | Allgood Hardware 203x19x11mm Lever Action Flush bolt, with coil spring, parallel movement radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48800FP] |
| 1.00 ea | SS48801F | Allgood Hardware 457x19mm Lever Action Flush bolt, with coil spring, parallel movement, radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48801FP] |
| 1.00 ea | SS7051 | Allgood Hardware 63x20x38mm easi-clean socket for wood or stone, grade 316, satin stainless finish |
| 1.00 ea | XX48800FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48800 flush bolts |
| 1.00 ea | XX48801FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48801 flush bolts |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 2.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |
| 1.00 ea | XX75574 | Allgood Secure 270x52x28mm surface mounted architectural electromagnet and armature for use on single door applications, 300kg holding force, MBS monitored and dual 12/24 DC voltage with 250ma current draw @ 12 volts and 125ma current draw @ 24 volts, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 60 minutes on metal doors |
| 1.00 ea | XX75574ZLC \* | Allgood Secure Z and L bracket armature assembly complete with architectural cover for use with XX75574 electromagnet. For use on inward opening doors only. |
| 1.00 ea | XX90009 \* | Access control to be supplied by others |

|  |
| --- |
| Total GBP: 969.48 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.43.01 | PM.DR.B1.SCR01.01 |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| Assume doors to have plain meeting stiles. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 03 -** | **BOH - DRT-01 - BWD/02/05/a/EHO/FD60/AC ( Frame Protection) - BLA** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 8.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 16.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 2.00 ea | XX98141S66 | Allgood Hardware, Figure 6, soffit bracket & template, satin stainless steel finish |
| 2.00 ea | XX98181S6 | Allgood Hardware Surface Mounted Electromagnetic Hold Open Overhead Door Closer, with swing free option, controlled closing, power size 4, universal fixings for timber and metal doors, supplied c/w black power transfer loop, frame mounted connection box and on/off switch, Certifire CF5517 listed to BS EN 1155, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on insulated metal doors, 10 year manufacturer warranty, satin stainless steel finish |
| 2.00 ea | SS1771SFF \* | Allgood Mode® 619x65x19mm mitred pull handle with concealed face fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 2.00 ea | XX30057 | Allgood Hardware 600x100mm PVC Sign 50mm letters 'push bar to open' (No Screws Supplied) |
| 4.00 ea | XX97950SS \* | Allgood Alite® FEKC 76øx1.2mm 'Fire Exit Keep Clear' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 2.00 ea | XX9329s \* | Allgood Hardware "Motorised" Touchbar 3 Point vertical rod panic bolt, suitable for wood, steel and aluminium doors, 840mm wide x 2650mm high, Certifire approved CF5516, CE/UKCA marked to EN1125 3-7-7-B-1-4-2-2-B-A, satin simulated stainless steel finish |
| 4.00 ea | XX97947SS | Allgood Alite® ADFKC 76øx1.2mm 'Automatic Fire Door Keep Clear' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 2.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |
| 2.00 ea | ZQ0062599 \* | Allgood Hardware 55x400x1.5mm Satin Stainless Steel Frame Protection Plate. Undrilled - SELF ADHESIVE BY OTHERS  NOMINAL SIZE ONLY - EXACT SIZES TBC FROM SITE |
| 1.00 ea | XX90009 \* | Access control to be supplied by others |

|  |
| --- |
| Total GBP: 2,680.45 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.38.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| We have assumed doors have plain meeting stiles.  PSU in sundries set |  |  |  |
| Make up of frame protection plate to be confirmed. Offcuts of tread plate to be considered. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 04 -** | **BOH - Leaf & half - DRT-04 - BWD/15/05/a/FD60/AC - NO KP** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 8.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 16.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | XX97948SS | Allgood Alite® FDKLS 76øx1.2mm 'Fire Door Keep Locked Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | SS48800F | Allgood Hardware 203x19x11mm Lever Action Flush bolt, with coil spring, parallel movement radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48800FP] |
| 1.00 ea | SS48801F | Allgood Hardware 457x19mm Lever Action Flush bolt, with coil spring, parallel movement, radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48801FP] |
| 1.00 ea | SS7051 | Allgood Hardware 63x20x38mm easi-clean socket for wood or stone, grade 316, satin stainless finish |
| 1.00 ea | XX48800FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48800 flush bolts |
| 1.00 ea | XX48801FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48801 flush bolts |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | XX75574 | Allgood Secure 270x52x28mm surface mounted architectural electromagnet and armature for use on single door applications, 300kg holding force, MBS monitored and dual 12/24 DC voltage with 250ma current draw @ 12 volts and 125ma current draw @ 24 volts, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 60 minutes on metal doors |
| 1.00 ea | XX75574ZLC \* | Allgood Secure Z and L bracket armature assembly complete with architectural cover for use with XX75574 electromagnet. For use on inward opening doors only. |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 1.00 ea | XX90009 \* | Access control to be supplied by others |

|  |
| --- |
| Total GBP: 535.20 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.00.34.01 | PM.DR.00.36.01 |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| Assumme Doors to have plain meeting stiles. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 05 -** | **BOH - Leaf & half - DRT-04 - BWD/15/05/a/FD30/AC** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 8.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 8.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S66 | Allgood Hardware, Figure 6, soffit bracket & template, satin stainless steel finish |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | XX97948SS | Allgood Alite® FDKLS 76øx1.2mm 'Fire Door Keep Locked Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | SS48800F | Allgood Hardware 203x19x11mm Lever Action Flush bolt, with coil spring, parallel movement radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48800FP] |
| 1.00 ea | SS48801F | Allgood Hardware 457x19mm Lever Action Flush bolt, with coil spring, parallel movement, radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48801FP] |
| 1.00 ea | SS7051 | Allgood Hardware 63x20x38mm easi-clean socket for wood or stone, grade 316, satin stainless finish |
| 1.00 ea | XX48800FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48800 flush bolts |
| 1.00 ea | XX48801FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48801 flush bolts |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 1.00 ea | XX75574 | Allgood Secure 270x52x28mm surface mounted architectural electromagnet and armature for use on single door applications, 300kg holding force, MBS monitored and dual 12/24 DC voltage with 250ma current draw @ 12 volts and 125ma current draw @ 24 volts, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 60 minutes on metal doors |
| 1.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |
| 1.00 ea | ZQ0062610 \* | 400x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread).  Final Site Size to be confirmed. |
| 1.00 ea | XX90009 \* | Access control to be supplied by others |

|  |
| --- |
| Total GBP: 794.84 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.BM.02.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| Assumme Doors to have plain meeting stiles. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 06 -** | **BOH - Leaf & half - DRT-04 - BWD/15/05/a/NFD** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 8.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | SS48800F | Allgood Hardware 203x19x11mm Lever Action Flush bolt, with coil spring, parallel movement radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48800FP] |
| 1.00 ea | SS48801F | Allgood Hardware 457x19mm Lever Action Flush bolt, with coil spring, parallel movement, radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48801FP] |
| 1.00 ea | SS7051 | Allgood Hardware 63x20x38mm easi-clean socket for wood or stone, grade 316, satin stainless finish |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 1.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |
| 1.00 ea | ZQ0062610 \* | 400x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread).  Final Site Size to be confirmed. |

|  |
| --- |
| Total GBP: 614.04 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.33.01 | PM.DR.B1.34.01 |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 07 -** | **FOH - Leaf & half - DRT-04 - FWD/15/05/c/FD30** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 8.00 ea | SS8066R | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with radius corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 8.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | XX98141S66 | Allgood Hardware, Figure 6, soffit bracket & template, satin stainless steel finish |
| 2.00 ea | SS8448 | Allgood Hardware 76mm circular 'Fire door keep locked' symbol, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, satin stainless steel finish |
| 2.00 ea | SS8449 | Allgood Hardware 76mm circular 'Fire door keep shut' symbol, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, satin stainless steel finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | SS48800F | Allgood Hardware 203x19x11mm Lever Action Flush bolt, with coil spring, parallel movement radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48800FP] |
| 1.00 ea | SS48801F | Allgood Hardware 457x19mm Lever Action Flush bolt, with coil spring, parallel movement, radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48801FP] |
| 1.00 ea | SS7051 | Allgood Hardware 63x20x38mm easi-clean socket for wood or stone, grade 316, satin stainless finish |
| 1.00 ea | XX48800FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48800 flush bolts |
| 1.00 ea | XX48801FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48801 flush bolts |
| 2.00 ea | ZQ0062599 \* | Allgood Hardware 55x400x1.5mm Satin Stainless Steel Frame Protection Plate. Undrilled - SELF ADHESIVE BY OTHERS  NOMINAL SIZE ONLY - EXACT SIZES TBC FROM SITE |
| 1.00 ea | SS2301 | Allgood Hardware 38x47mm Heavy Duty Circular Floor Mounted Door Stop, grade 316, 25 year manufacturing warranty, satin stainless steel finish |
| 1.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |
| 1.00 ea | ZQ0062610 \* | 400x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread).  Final Site Size to be confirmed. |

|  |
| --- |
| Total GBP: 798.37 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.BM.14.02 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| Assume doors to have plain meeting stiles. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 08 -** | **BOH - Leaf & half - DRT-04 - BWD/15/05/a/FD60 (a) Frame Protection** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 8.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 16.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | XX97948SS | Allgood Alite® FDKLS 76øx1.2mm 'Fire Door Keep Locked Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | SS48800F | Allgood Hardware 203x19x11mm Lever Action Flush bolt, with coil spring, parallel movement radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48800FP] |
| 1.00 ea | SS48801F | Allgood Hardware 457x19mm Lever Action Flush bolt, with coil spring, parallel movement, radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48801FP] |
| 1.00 ea | SS7051 | Allgood Hardware 63x20x38mm easi-clean socket for wood or stone, grade 316, satin stainless finish |
| 1.00 ea | XX48800FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48800 flush bolts |
| 1.00 ea | XX48801FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48801 flush bolts |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 2.00 ea | ZQ0062599 \* | Allgood Hardware 55x400x1.5mm Satin Stainless Steel Frame Protection Plate. Undrilled - SELF ADHESIVE BY OTHERS  NOMINAL SIZE ONLY - EXACT SIZES TBC FROM SITE |
| 1.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |
| 1.00 ea | ZQ0062610 \* | 400x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread).  Final Site Size to be confirmed. |

|  |
| --- |
| Total GBP: 679.16 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.BM.11A.01 | PM.DR.BM.11A.02 | PM.DR.BM.13.01 | PM.DR.BM.PL01 |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| Assume doors to have plain meeting stiles.  Make up of frame protection plate to be confirmed. Offcuts of tread plate to be considered. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 12 -** | **FOH - Single cleaners cupboard DRT-02a - FWD/01/07/CL/FD30** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 3.00 ea | SS8066R | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with radius corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 3.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | SN9133N | Allgood Hardware 280x46x33mm Concealed Overhead Door closer, with finished track & arm for Single Action Doors, adjustable power 2-4, closing force, latch action & cushion stop, Certifire approved CF6022 for use on up to 60 minute timber fire doors & CE Marked to BS EN1154: 3-8-4/2-1-1-3, 10 year manufacturer warranty, SNP finish |
| 1.00 ea | XX9133FPN \* | Allgood Hardware Size 2-4 Concealed Cam Closer Intumescent Pack for use on up to 60 minute timber fire doors to suit 9133N |
| 1.00 ea | SN7319AM \* | Allgood Hardware 'A' 60mm (30/30) length Euro Profile Cylinder & turn, independently tested to BS EN 1303:2015 classification 1/6/0/B\*1/0/C/6/D, trademark protection 6 pin cylinder with solid and lateral profile pins, c/w “anti-Bump”, “anti-pick”, “anti-drill” and “anti-pull” protection, 2 keyed, under master key, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors, satin nickel finish |
| 1.00 ea | SS7286F60 | Allgood Hardware 92x60mm backset HL series profile cylinder mortice deadlock case only, single throw 20mm Stainless Steel deadbolt, rounded forend & strike CE Marked to BS EN: 12209 3/X/8/1/0/G/2/B/A/0/0 Certifire approved CF347 for use on 90 minute timber fire doors and up to 240 minutes for metal fire doors, 10 year manufacturing warranty, satin stainless steel finish |
| 1.00 ea | XX7286FP6 | Allgood Hardware intumescent Lock Fire Pack 7286 60mm backset Series |
| 2.00 ea | SS796Q | Allgood Modric® 50x4mm Circular Escutcheon for Euro Profile Cylinder, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and for up to 240 minutes on metal doors, grade 316, 25 year manufacturing warranty, satin stainless steel finish |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 2.00 ea | SS8449 | Allgood Hardware 76mm circular 'Fire door keep shut' symbol, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, satin stainless steel finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | SS8455 \* | Allgood Modric® 76ømmx2.5mm 'Cleaners - Mop & Bucket graphic' sign with torx screw fixings, satin stainless steel finish |

|  |
| --- |
| Total GBP: 466.25 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.00.16.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 15 -** | **BOH - Single access controlled door w/levers - DRT-02a - FWD/01/05/c/FD60** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 4.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 1.00 ea | XX9943NFP \* | Allgood Hardware intumescent Redlock Fire Pack 99 Series Redlocks |
| 8.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | SS9938F \* | Allgood Hardware finished forend & striking plate for Redlocks, 9941/9942/9943/9944/9945/9946, satin stainless steel finish |
| 1.00 ea | SS9943F5 \* | Allgood Secure 145x114x72 solenoid controlled Redlock® mortice lock case only, pierced for euro profile cylinder with both lever handles controlled, fail secure, twin monitored latchbolt and anti-thrust bolt, 12v DC, 200mA solenoid current draw, 72mm backset, 72mm centres, 8mm follower, Reversible latchbolt and strike plate, radius outer forend, UL Listed R27527 UL10C, compliant with ANSI 115.1, suits standard preparation for metal doors, Allgood Cylinders recommended in use to ensure compatibility, 10 year mechanical warranty, satin stainless steel finish |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 pr | XX97423SSN | Allgood Alite® 127 x 64mm x 19mmØ Straight lever handles, on Quadaxial® 50Ø x 4mm concealed fixing roses (tested to 1 million cycles), independently tested to BS EN 1906 4/7/-/1/0/3/0/U, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, suitable for doors 35-54mm, grade 304, satin stainless steel finish |
| 2.00 ea | SP0048 | 4 no 6 x 1/2 screws for use with Quadaxial roses |
| 1.00 ea | SN7320BM \* | Allgood Hardware 'B' 45mm (35/10) length Euro Profile Single cylinder, independently tested to BS EN 1303:2015 classification 1/6/0/B\*1/0/C/6/D, trademark protection 6 pin cylinder with solid and lateral profile pins, c/w “anti-Bump”, “anti-pick”, “anti-drill” and “anti-pull” protection, 2 keyed, under master key, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors, satin nickel plated finish |
| 1.00 ea | XX97876SS | Allgood Alite® Cylinder Rose, 50mm diameter concealed with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 60 minute timber doors, satin stainless steel finish |
| 1.00 ea | XX79053N | Allgood Secure Concealed Door Loop with square ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors, silver finish, [For Fire Pack Order XX79053FP] |
| 2.00 ea | XX79053FP | Allgood Secure Concealed Door Loop fire pack |
| 1.00 ea | XX9069T | Allgood Hardware 8mm HT singletite split spindle for 40-64mm doors for use with knobs, levers & Allgood split follower locks |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |
| 1.00 ea | XX90009 \* | Access control to be supplied by others |

|  |
| --- |
| Total GBP: 1,003.11 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.PL06.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| Lever handles and maglock not compatible.  We have therefore allowed for a solenoid mortice lock case.  Please confirm. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 17 -** | **BOH - Single circulation door - DRT-02 - WD/01/05 - NFD** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 3.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 1.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |

|  |
| --- |
| Total GBP: 414.50 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.37.01 | PM.DR.BM.SCR02.01 |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 18 -** | **BOH - Single cleaners cupboard - DRT-02 - BWD/01/07/CL/FD30** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 1.00 ea | SS7631F \* | Spare Radius Strike Plate for Bathroom/Sashlock New 76 Series SS7608FS60/SS7679FS60 |
| 4.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 4.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SN7319AM \* | Allgood Hardware 'A' 60mm (30/30) length Euro Profile Cylinder & turn, independently tested to BS EN 1303:2015 classification 1/6/0/B\*1/0/C/6/D, trademark protection 6 pin cylinder with solid and lateral profile pins, c/w “anti-Bump”, “anti-pick”, “anti-drill” and “anti-pull” protection, 2 keyed, under master key, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors, satin nickel finish |
| 1.00 ea | SS7679FN60 | Allgood Hardware 93x60mm backset profile cylinder mortice lock case only, heavy sprung for levers, double throw deadbolt, CE Marked to BS EN 12209 3/X/8/1/0/G/2/B/C/2/0, Certifire approved CF5899 for use up to 120 minutes on timber fire doors and 240 minute metal fire doors, radius forend & square strike, satin stainless steel finish |
| 1.00 ea | XX7679FP1 | Allgood Hardware intumescent Pack for 76 Series 60mm Backset TFD30, TFD60 |
| 1.00 pr | XX97423SSN | Allgood Alite® 127 x 64mm x 19mmØ Straight lever handles, on Quadaxial® 50Ø x 4mm concealed fixing roses (tested to 1 million cycles), independently tested to BS EN 1906 4/7/-/1/0/3/0/U, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, suitable for doors 35-54mm, grade 304, satin stainless steel finish |
| 2.00 ea | XX97876SS | Allgood Alite® Cylinder Rose, 50mm diameter concealed with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 60 minute timber doors, satin stainless steel finish |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | XX97955SS | Allgood Alite® 76øx1.2mm 'Cleaners' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |

|  |
| --- |
| Total GBP: 456.79 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.41.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 19 -** | **BOH - Single circulation door - DRT-02 - BWD/01/05/a/FD30** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 4.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 4.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |

|  |
| --- |
| Total GBP: 427.12 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.ST05.02 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 20 -** | **BOH - Single lockable door w/levers - DRT-02 - BWD/01/09/a/FD30** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 1.00 ea | SS7631F \* | Spare Radius Strike Plate for Bathroom/Sashlock New 76 Series SS7608FS60/SS7679FS60 |
| 4.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 4.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | XX98141S66 | Allgood Hardware, Figure 6, soffit bracket & template, satin stainless steel finish |
| 1.00 ea | SS7679FN60 | Allgood Hardware 93x60mm backset profile cylinder mortice lock case only, heavy sprung for levers, double throw deadbolt, CE Marked to BS EN 12209 3/X/8/1/0/G/2/B/C/2/0, Certifire approved CF5899 for use up to 120 minutes on timber fire doors and 240 minute metal fire doors, radius forend & square strike, satin stainless steel finish |
| 1.00 ea | XX7679FP1 | Allgood Hardware intumescent Pack for 76 Series 60mm Backset TFD30, TFD60 |
| 1.00 pr | XX97423SSN | Allgood Alite® 127 x 64mm x 19mmØ Straight lever handles, on Quadaxial® 50Ø x 4mm concealed fixing roses (tested to 1 million cycles), independently tested to BS EN 1906 4/7/-/1/0/3/0/U, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, suitable for doors 35-54mm, grade 304, satin stainless steel finish |
| 1.00 ea | SN7319AM \* | Allgood Hardware 'A' 60mm (30/30) length Euro Profile Cylinder & turn, independently tested to BS EN 1303:2015 classification 1/6/0/B\*1/0/C/6/D, trademark protection 6 pin cylinder with solid and lateral profile pins, c/w “anti-Bump”, “anti-pick”, “anti-drill” and “anti-pull” protection, 2 keyed, under master key, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors, satin nickel finish |
| 2.00 ea | XX97876SS | Allgood Alite® Cylinder Rose, 50mm diameter concealed with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 60 minute timber doors, satin stainless steel finish |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |

|  |
| --- |
| Total GBP: 454.62 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.46.01 | PM.DR.B1.47.01 | PM.DR.B1.48.01 | PM.DR.B1.49.01 |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 21 -** | **BOH - Single lockable door w/levers - DRT-02 - BWD/01/09/a/FD60** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 1.00 ea | SS7631F \* | Spare Radius Strike Plate for Bathroom/Sashlock New 76 Series SS7608FS60/SS7679FS60 |
| 4.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 8.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SN7319AM \* | Allgood Hardware 'A' 60mm (30/30) length Euro Profile Cylinder & turn, independently tested to BS EN 1303:2015 classification 1/6/0/B\*1/0/C/6/D, trademark protection 6 pin cylinder with solid and lateral profile pins, c/w “anti-Bump”, “anti-pick”, “anti-drill” and “anti-pull” protection, 2 keyed, under master key, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors, satin nickel finish |
| 1.00 ea | SS7679FN60 | Allgood Hardware 93x60mm backset profile cylinder mortice lock case only, heavy sprung for levers, double throw deadbolt, CE Marked to BS EN 12209 3/X/8/1/0/G/2/B/C/2/0, Certifire approved CF5899 for use up to 120 minutes on timber fire doors and 240 minute metal fire doors, radius forend & square strike, satin stainless steel finish |
| 1.00 ea | XX7679FP1 | Allgood Hardware intumescent Pack for 76 Series 60mm Backset TFD30, TFD60 |
| 1.00 pr | XX97423SSN | Allgood Alite® 127 x 64mm x 19mmØ Straight lever handles, on Quadaxial® 50Ø x 4mm concealed fixing roses (tested to 1 million cycles), independently tested to BS EN 1906 4/7/-/1/0/3/0/U, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, suitable for doors 35-54mm, grade 304, satin stainless steel finish |
| 2.00 ea | XX97876SS | Allgood Alite® Cylinder Rose, 50mm diameter concealed with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 60 minute timber doors, satin stainless steel finish |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |

|  |
| --- |
| Total GBP: 459.06 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.51.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 22 -** | **BOH - Double access controlled circulation - DRT-01 - BWD/02/05/a/EHO/FD60/AC/1** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 8.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 16.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98181S6 | Allgood Hardware Surface Mounted Electromagnetic Hold Open Overhead Door Closer, with swing free option, controlled closing, power size 4, universal fixings for timber and metal doors, supplied c/w black power transfer loop, frame mounted connection box and on/off switch, Certifire CF5517 listed to BS EN 1155, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on insulated metal doors, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | XX97947SS | Allgood Alite® ADFKC 76øx1.2mm 'Automatic Fire Door Keep Clear' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 2.00 ea | XX97948SS | Allgood Alite® FDKLS 76øx1.2mm 'Fire Door Keep Locked Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | SS48800F | Allgood Hardware 203x19x11mm Lever Action Flush bolt, with coil spring, parallel movement radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48800FP] |
| 1.00 ea | SS48801F | Allgood Hardware 457x19mm Lever Action Flush bolt, with coil spring, parallel movement, radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48801FP] |
| 1.00 ea | SS7051 | Allgood Hardware 63x20x38mm easi-clean socket for wood or stone, grade 316, satin stainless finish |
| 1.00 ea | XX48800FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48800 flush bolts |
| 1.00 ea | XX48801FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48801 flush bolts |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 1.00 ea | XX75574 | Allgood Secure 270x52x28mm surface mounted architectural electromagnet and armature for use on single door applications, 300kg holding force, MBS monitored and dual 12/24 DC voltage with 250ma current draw @ 12 volts and 125ma current draw @ 24 volts, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 60 minutes on metal doors |
| 1.00 ea | XX75574ZLC \* | Allgood Secure Z and L bracket armature assembly complete with architectural cover for use with XX75574 electromagnet. For use on inward opening doors only. |
| 2.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |
| 1.00 ea | XX90009 \* | Access control to be supplied by others |

|  |
| --- |
| Total GBP: 1,174.30 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.07.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| We have assumed doors have plain meeting stiles.  Make up of frame protection plate to be confirmed. Offcuts of tread plate to be considered. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 23 -** | **BOH - Double access controlled circulation door - DRT-01 - BWD/02/05/a/EHO/FD60/AC/2 - nds ( Frame Protection )** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 8.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 16.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S66 | Allgood Hardware, Figure 6, soffit bracket & template, satin stainless steel finish |
| 1.00 ea | XX98181S6 | Allgood Hardware Surface Mounted Electromagnetic Hold Open Overhead Door Closer, with swing free option, controlled closing, power size 4, universal fixings for timber and metal doors, supplied c/w black power transfer loop, frame mounted connection box and on/off switch, Certifire CF5517 listed to BS EN 1155, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on insulated metal doors, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | XX97948SS | Allgood Alite® FDKLS 76øx1.2mm 'Fire Door Keep Locked Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | SS48800F | Allgood Hardware 203x19x11mm Lever Action Flush bolt, with coil spring, parallel movement radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48800FP] |
| 1.00 ea | SS48801F | Allgood Hardware 457x19mm Lever Action Flush bolt, with coil spring, parallel movement, radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48801FP] |
| 1.00 ea | SS7051 | Allgood Hardware 63x20x38mm easi-clean socket for wood or stone, grade 316, satin stainless finish |
| 1.00 ea | XX48800FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48800 flush bolts |
| 1.00 ea | XX48801FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48801 flush bolts |
| 2.00 ea | XX97947SS | Allgood Alite® ADFKC 76øx1.2mm 'Automatic Fire Door Keep Clear' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 2.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |
| 1.00 ea | XX75574 | Allgood Secure 270x52x28mm surface mounted architectural electromagnet and armature for use on single door applications, 300kg holding force, MBS monitored and dual 12/24 DC voltage with 250ma current draw @ 12 volts and 125ma current draw @ 24 volts, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 60 minutes on metal doors |
| 1.00 ea | XX75574ZLC \* | Allgood Secure Z and L bracket armature assembly complete with architectural cover for use with XX75574 electromagnet. For use on inward opening doors only. |
| 2.00 ea | ZQ0062599 \* | Allgood Hardware 55x400x1.5mm Satin Stainless Steel Frame Protection Plate. Undrilled - SELF ADHESIVE BY OTHERS  NOMINAL SIZE ONLY - EXACT SIZES TBC FROM SITE |
| 1.00 ea | XX90009 \* | Access control to be supplied by others |

|  |
| --- |
| Total GBP: 1,197.70 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.07.02 | PM.DR.B1.07.03 |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| Assume doors to have plain meeting stiles.  Make up of frame protection plate to be confirmed. Offcuts of tread plate to be considered. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 24 -** | **BOH - Double circulation door - DRT-01 - BWD/02/05/a/EHO/FD60/AC/a (Frame Protection)** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 8.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 16.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98181S6 | Allgood Hardware Surface Mounted Electromagnetic Hold Open Overhead Door Closer, with swing free option, controlled closing, power size 4, universal fixings for timber and metal doors, supplied c/w black power transfer loop, frame mounted connection box and on/off switch, Certifire CF5517 listed to BS EN 1155, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on insulated metal doors, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | XX97947SS | Allgood Alite® ADFKC 76øx1.2mm 'Automatic Fire Door Keep Clear' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 2.00 ea | XX97948SS | Allgood Alite® FDKLS 76øx1.2mm 'Fire Door Keep Locked Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | SS48800F | Allgood Hardware 203x19x11mm Lever Action Flush bolt, with coil spring, parallel movement radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48800FP] |
| 1.00 ea | SS48801F | Allgood Hardware 457x19mm Lever Action Flush bolt, with coil spring, parallel movement, radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48801FP] |
| 1.00 ea | SS7051 | Allgood Hardware 63x20x38mm easi-clean socket for wood or stone, grade 316, satin stainless finish |
| 1.00 ea | XX48800FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48800 flush bolts |
| 1.00 ea | XX48801FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48801 flush bolts |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 2.00 ea | ZQ0062599 \* | Allgood Hardware 55x400x1.5mm Satin Stainless Steel Frame Protection Plate. Undrilled - SELF ADHESIVE BY OTHERS  NOMINAL SIZE ONLY - EXACT SIZES TBC FROM SITE |
| 2.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |
| 1.00 ea | XX75574 | Allgood Secure 270x52x28mm surface mounted architectural electromagnet and armature for use on single door applications, 300kg holding force, MBS monitored and dual 12/24 DC voltage with 250ma current draw @ 12 volts and 125ma current draw @ 24 volts, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 60 minutes on metal doors |
| 1.00 ea | XX75574ZLC \* | Allgood Secure Z and L bracket armature assembly complete with architectural cover for use with XX75574 electromagnet. For use on inward opening doors only. |
| 1.00 ea | XX90009 \* | Access control to be supplied by others |

|  |
| --- |
| Total GBP: 1,197.62 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.BM.10.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| Make up of frame protection plate to be confirmed. Offcuts of tread plate to be considered. |  |  |  |
| We have assumed doors have plain meeting stiles. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 25 -** | **BOH - Double circulation door - DRT-01 - BWD/02/05/a/FD30 ( Frame Protection)** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 8.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 8.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | XX98141S66 | Allgood Hardware, Figure 6, soffit bracket & template, satin stainless steel finish |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | XX97948SS | Allgood Alite® FDKLS 76øx1.2mm 'Fire Door Keep Locked Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | SS48800F | Allgood Hardware 203x19x11mm Lever Action Flush bolt, with coil spring, parallel movement radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48800FP] |
| 1.00 ea | SS48801F | Allgood Hardware 457x19mm Lever Action Flush bolt, with coil spring, parallel movement, radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48801FP] |
| 1.00 ea | SS7051 | Allgood Hardware 63x20x38mm easi-clean socket for wood or stone, grade 316, satin stainless finish |
| 1.00 ea | XX48800FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48800 flush bolts |
| 1.00 ea | XX48801FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48801 flush bolts |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 2.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |
| 2.00 ea | ZQ0062599 \* | Allgood Hardware 55x400x1.5mm Satin Stainless Steel Frame Protection Plate. Undrilled - SELF ADHESIVE BY OTHERS  NOMINAL SIZE ONLY - EXACT SIZES TBC FROM SITE |

|  |
| --- |
| Total GBP: 769.10 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.BM.14.01 | PM.DR.BM.15.01 |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| Assume doors to have plain meeting stiles.  Make up of frame protection plate to be confirmed. Offcuts of tread plate to be considered. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 26 -** | **BOH - Double circulation door - DRT-01 - BWD/02/05/a/FD60/2 - 1ds** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 8.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 16.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | XX97948SS | Allgood Alite® FDKLS 76øx1.2mm 'Fire Door Keep Locked Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | SS48800F | Allgood Hardware 203x19x11mm Lever Action Flush bolt, with coil spring, parallel movement radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48800FP] |
| 1.00 ea | SS48801F | Allgood Hardware 457x19mm Lever Action Flush bolt, with coil spring, parallel movement, radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48801FP] |
| 1.00 ea | SS7051 | Allgood Hardware 63x20x38mm easi-clean socket for wood or stone, grade 316, satin stainless finish |
| 1.00 ea | XX48800FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48800 flush bolts |
| 1.00 ea | XX48801FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48801 flush bolts |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 2.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |

|  |
| --- |
| Total GBP: 749.17 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.31.02 | PM.DR.B1.53.01 | PM.DR.B1.PL03A.01 | PM.DR.B1.PL08.01 | PM.DR.B1.PL09.01 | PM.DR.B1.PL15.01 |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| We have assumed doors have plain meeting stiles. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 27 -** | **BOH - Double circulation door - DRT-01 - BWD/02/05/a/FD60/1 - nds** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 8.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 16.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | XX97948SS | Allgood Alite® FDKLS 76øx1.2mm 'Fire Door Keep Locked Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | SS48800F | Allgood Hardware 203x19x11mm Lever Action Flush bolt, with coil spring, parallel movement radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48800FP] |
| 1.00 ea | SS48801F | Allgood Hardware 457x19mm Lever Action Flush bolt, with coil spring, parallel movement, radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48801FP] |
| 1.00 ea | SS7051 | Allgood Hardware 63x20x38mm easi-clean socket for wood or stone, grade 316, satin stainless finish |
| 1.00 ea | XX48800FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48800 flush bolts |
| 1.00 ea | XX48801FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48801 flush bolts |
| 2.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |

|  |
| --- |
| Total GBP: 743.60 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.PL04.01 | PM.DR.B1.PL13.01 | PM.DR.B1.PL14.01 | PM.DR.B1.PL18.01 | PM.DR.B1.PL19.01 | PM.DR.B1.PL20.01 |
| PM.DR.B1.PL22.02 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| We have assumed doors have plain meeting stiles. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 28 -** | **FOH - Single circulation door - DRT-02 - FWD/01/05/c** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 4.00 ea | SS8066R | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with radius corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 1.00 ea | SN9133N | Allgood Hardware 280x46x33mm Concealed Overhead Door closer, with finished track & arm for Single Action Doors, adjustable power 2-4, closing force, latch action & cushion stop, Certifire approved CF6022 for use on up to 60 minute timber fire doors & CE Marked to BS EN1154: 3-8-4/2-1-1-3, 10 year manufacturer warranty, SNP finish |
| 1.00 ea | SS1761 | Allgood Mode® 700x67x19mm entrance pull handle with bolt through fixings at 600mm centres, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | SS2301 | Allgood Hardware 38x47mm Heavy Duty Circular Floor Mounted Door Stop, grade 316, 25 year manufacturing warranty, satin stainless steel finish |
| 1.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |

|  |
| --- |
| Total GBP: 543.16 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.00.22.03 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 29 -** | **BOH - Single circulation door - DRT-02 - BWD/01/05/a/FD60** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 4.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 8.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 1.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |

|  |
| --- |
| Total GBP: 431.64 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.PL22.01 | PM.DR.B1.ST06.01 | PM.DR.BM.05.01 | PM.DR.BM.09.01 | PM.DR.BM.16.01 | PM.DR.BM.SCR03.02 |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| PM.DR.B1.PL21.02 - Components subject to approval by door manufacturer to ensure compliance with security rating. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 30 -** | **BOH - Single access controlled door w/levers - DRT-02 - BWD/01/09/a/FD30/AC** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 4.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 1.00 ea | XX9943NFP \* | Allgood Hardware intumescent Redlock Fire Pack 99 Series Redlocks |
| 4.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | XX98141S66 | Allgood Hardware, Figure 6, soffit bracket & template, satin stainless steel finish |
| 1.00 ea | SS9938F \* | Allgood Hardware finished forend & striking plate for Redlocks, 9941/9942/9943/9944/9945/9946, satin stainless steel finish |
| 1.00 ea | SS9943F5 \* | Allgood Secure 145x114x72 solenoid controlled Redlock® mortice lock case only, pierced for euro profile cylinder with both lever handles controlled, fail secure, twin monitored latchbolt and anti-thrust bolt, 12v DC, 200mA solenoid current draw, 72mm backset, 72mm centres, 8mm follower, Reversible latchbolt and strike plate, radius outer forend, UL Listed R27527 UL10C, compliant with ANSI 115.1, suits standard preparation for metal doors, Allgood Cylinders recommended in use to ensure compatibility, 10 year mechanical warranty, satin stainless steel finish |
| 1.00 pr | XX97423SSN | Allgood Alite® 127 x 64mm x 19mmØ Straight lever handles, on Quadaxial® 50Ø x 4mm concealed fixing roses (tested to 1 million cycles), independently tested to BS EN 1906 4/7/-/1/0/3/0/U, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, suitable for doors 35-54mm, grade 304, satin stainless steel finish |
| 2.00 ea | SP0048 | 4 no 6 x 1/2 screws for use with Quadaxial roses |
| 1.00 ea | XX79053N | Allgood Secure Concealed Door Loop with square ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors, silver finish, [For Fire Pack Order XX79053FP] |
| 1.00 ea | XX79053FP | Allgood Secure Concealed Door Loop fire pack |
| 1.00 ea | SN7320AM \* | Allgood Hardware 'A' 40mm (30/10) length Euro Profile Single Cylinder, independently tested to BS EN 1303:2015 classification 1/6/0/B\*1/0/C/6/D, trademark protection 6 pin cylinder with solid and lateral profile pins, c/w “anti-Bump”, “anti-pick”, “anti-drill” and “anti-pull” protection, 2 keyed, under master key, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors, satin nickel plated finish |
| 1.00 ea | XX97876SS | Allgood Alite® Cylinder Rose, 50mm diameter concealed with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 60 minute timber doors, satin stainless steel finish |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 1.00 ea | XX9069T | Allgood Hardware 8mm HT singletite split spindle for 40-64mm doors for use with knobs, levers & Allgood split follower locks |
| 1.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |
| 1.00 ea | XX90009 \* | Access control to be supplied by others |

|  |
| --- |
| Total GBP: 975.07 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.44.01 | PM.DR.B1.45.01 |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| Please use screw pack (SP0048) supplied, to fix through the horizontal fixings points on the lever sub-roses. (Please refer to Redlock fixing instructions, for further information). |  |  |  |
| Allgood Solenoid Redocks require both cable route and a suitable cable transfer loop to allow the lock cable to be routed from the door to the frame. Timber doors will require a hole of 8 mm diameter to be bored through the door leaf from the lock position to the cable transfer loop position. It is recommended that all fire rated door sets are fully assessed by the door manufacturer to ensure that cable route holes do not undermine the integrity of the door set during fire conditions. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 31 -** | **BOH - Single access controlled circulation door - DRT-02 - BWD/01/05/a/FD60/AC** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 4.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 8.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 1.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |
| 1.00 ea | XX75574 | Allgood Secure 270x52x28mm surface mounted architectural electromagnet and armature for use on single door applications, 300kg holding force, MBS monitored and dual 12/24 DC voltage with 250ma current draw @ 12 volts and 125ma current draw @ 24 volts, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 60 minutes on metal doors |
| 1.00 ea | XX75574ZLC \* | Allgood Secure Z and L bracket armature assembly complete with architectural cover for use with XX75574 electromagnet. For use on inward opening doors only. |
| 1.00 ea | XX90009 \* | Access control to be supplied by others |

|  |
| --- |
| Total GBP: 660.99 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.BM.SCR07.01 | PM.DR.BM.ST05.01 |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 35 -** | **BOH - Single circulation door - DRT-02a - BWD/01/05/a** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 3.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |

|  |
| --- |
| Total GBP: 192.84 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.00.33.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 37 -** | **BOH - Single female entrance door - DRT-02a - BWD/01/05/a/F/FD30 - 1M High P/P** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 3.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 3.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069803 \* | Allgood Hardware 1000x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixing -  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | XX97933SS | Allgood Alite® 76øx1.2mm 'Female' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |

|  |
| --- |
| Total GBP: 195.42 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.26.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 38 -** | **BOH - Single male entrance door - DRT-02a - BWD/01/05/a/M/FD30 - 1M High P/P** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 3.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 3.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069803 \* | Allgood Hardware 1000x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixing -  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | XX97932SS | Allgood Alite® 76øx1.2mm 'Male' Symbol Disc, with screw fixings, grade 430, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, satin stainless steel finish, Horizontal Grain |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |

|  |
| --- |
| Total GBP: 195.42 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.27.04 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 41 -** | **FOH - Single lockable circulation door - DRT-02a - FWD/01/06/c/FD60** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 4.00 ea | SS8066R | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with radius corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 1.00 ea | SN9133N | Allgood Hardware 280x46x33mm Concealed Overhead Door closer, with finished track & arm for Single Action Doors, adjustable power 2-4, closing force, latch action & cushion stop, Certifire approved CF6022 for use on up to 60 minute timber fire doors & CE Marked to BS EN1154: 3-8-4/2-1-1-3, 10 year manufacturer warranty, SNP finish |
| 8.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX9133FPN \* | Allgood Hardware Size 2-4 Concealed Cam Closer Intumescent Pack for use on up to 60 minute timber fire doors to suit 9133N |
| 1.00 ea | SN7319BM \* | Allgood Hardware 'B' 70mm (35/35) length Euro Profile Cylinder & turn, independently tested to BS EN 1303:2015 classification 1/6/0/B\*1/0/C/6/D, trademark protection 6 pin cylinder with solid and lateral profile pins, c/w “anti-Bump”, “anti-pick”, “anti-drill” and “anti-pull” protection, 2 keyed, under master key, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors, satin nickel plated finish |
| 1.00 ea | SS7286F60 | Allgood Hardware 92x60mm backset HL series profile cylinder mortice deadlock case only, single throw 20mm Stainless Steel deadbolt, rounded forend & strike CE Marked to BS EN: 12209 3/X/8/1/0/G/2/B/A/0/0 Certifire approved CF347 for use on 90 minute timber fire doors and up to 240 minutes for metal fire doors, 10 year manufacturing warranty, satin stainless steel finish |
| 1.00 ea | XX7286FP6 | Allgood Hardware intumescent Lock Fire Pack 7286 60mm backset Series |
| 1.00 ea | SS1761 | Allgood Mode® 700x67x19mm entrance pull handle with bolt through fixings at 600mm centres, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | SS796Q | Allgood Modric® 50x4mm Circular Escutcheon for Euro Profile Cylinder, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and for up to 240 minutes on metal doors, grade 316, 25 year manufacturing warranty, satin stainless steel finish |
| 2.00 ea | SS8449 | Allgood Hardware 76mm circular 'Fire door keep shut' symbol, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, satin stainless steel finish |
| 1.00 ea | SS2301 | Allgood Hardware 38x47mm Heavy Duty Circular Floor Mounted Door Stop, grade 316, 25 year manufacturing warranty, satin stainless steel finish |

|  |
| --- |
| Total GBP: 496.75 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.00.46.01 | PM.DR.00.59.01 |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 42 -** | **FOH - Single first aid door - DRT-02a - FWD/01/08/c/FA/FD60** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 4.00 ea | SS8066R | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with radius corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 1.00 ea | ZQ0066963 \* | FD60 Intumescent pack to suit G8023 cubicle deadlock. |
| 8.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | ZQ0071750 \* | G8023 - 76mm Cubicle deadlock. 57mm Backset. 8mm Brass Follower. CE Marked. Fire Tested to BSEN 1634-1:2000. Radius Forend & Strike Plate - Satin Stainless Steel Finish |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | SS771Q2529 | Allgood Modric® 37x17x18mm WC Turn on 50mmø x 4mm rose, complete with emergency release rose with indicator and 5-8mm spindle, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 60 minute timber doors, 25 year manufacturing warranty, satin stainless steel finish. |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | SS8449 | Allgood Hardware 76mm circular 'Fire door keep shut' symbol, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, satin stainless steel finish |
| 1.00 ea | SS8459 \* | Allgood Modric® 76mm 'First Aid' circular symbol, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, satin stainless steel finish |
| 1.00 ea | SS6541 | Allgood Modric® 14mmø x 38mm coat hook with pin and concealed fixing, grade 316, 25 year manufacturer warranty,satin stainless steel finish |

|  |
| --- |
| Total GBP: 382.62 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.00.57.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 44 -** | **BOH - Leaf & half circulation door - DRT-04 - BWD/15/05/a/FD60** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 1.00 ea | SS7636F \* | Spare Radius Strike Plate for Deadlock New 76 Series SS7686FS60 |
| 8.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 16.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SN7319BM \* | Allgood Hardware 'B' 70mm (35/35) length Euro Profile Cylinder & turn, independently tested to BS EN 1303:2015 classification 1/6/0/B\*1/0/C/6/D, trademark protection 6 pin cylinder with solid and lateral profile pins, c/w “anti-Bump”, “anti-pick”, “anti-drill” and “anti-pull” protection, 2 keyed, under master key, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors, satin nickel plated finish |
| 1.00 ea | SS7686FN60 | Allgood Hardware 93x60mm backset profile cylinder mortice deadlock case only, double throw 20mm deadbolt, CE Marked to BS EN 12209 3/X/8/1/0/G/2/B/C/0/0, Certifire approved CF5899 for use up to 120 minutes on timber fire doors and 240 minute metal fire doors, radius forend & square strike, satin stainless steel finish |
| 1.00 ea | XX7679FP1 | Allgood Hardware intumescent Pack for 76 Series 60mm Backset TFD30, TFD60 |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 2.00 ea | XX97876SS | Allgood Alite® Cylinder Rose, 50mm diameter concealed with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 60 minute timber doors, satin stainless steel finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | SS48800F | Allgood Hardware 203x19x11mm Lever Action Flush bolt, with coil spring, parallel movement radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48800FP] |
| 1.00 ea | SS48801F | Allgood Hardware 457x19mm Lever Action Flush bolt, with coil spring, parallel movement, radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48801FP] |
| 1.00 ea | XX48800FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48800 flush bolts |
| 1.00 ea | XX48801FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48801 flush bolts |
| 1.00 ea | SS7051 | Allgood Hardware 63x20x38mm easi-clean socket for wood or stone, grade 316, satin stainless finish |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 2.00 ea | XX97948SS | Allgood Alite® FDKLS 76øx1.2mm 'Fire Door Keep Locked Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 1.00 ea | XX90010 \* | See Remarks |
| 1.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |
| 1.00 ea | ZQ0062610 \* | 400x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread).  Final Site Size to be confirmed. |

|  |
| --- |
| Total GBP: 747.05 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.PL11.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| Is manual locking required? |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 45 -** | **FOH - Leaf & half access controlled circulation - DRT-04a - FWD/15/05/c/FD30 - BLA** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 8.00 ea | SS8066R | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with radius corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 1.00 ea | XX10508FPN | Allgood Hardware intumescent pack for 10508 jamb mounted closer, suitable for timber doors in FD30/60 applications |
| 16.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | SC10508 | Allgood Hardware fully concealed jamb fixed door closer, CE Marked to BS EN: 1154 classification 3-8-3-1-1-3, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 240 minutes on metal doors, satin chrome plated finish (For Fire Pack not supplied order XX10508FPN) |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 2.00 ea | SS1761 | Allgood Mode® 700x67x19mm entrance pull handle with bolt through fixings at 600mm centres, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 4.00 ea | SS8449 | Allgood Hardware 76mm circular 'Fire door keep shut' symbol, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, satin stainless steel finish |
| 2.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | SS2301 | Allgood Hardware 38x47mm Heavy Duty Circular Floor Mounted Door Stop, grade 316, 25 year manufacturing warranty, satin stainless steel finish |
| 1.00 ea | ZQ0062637 \* | Allgood Hardware 900x450x1.5mm Satin Stainless Steel Kick Plate. Undrilled.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | ZQ0062638 \* | Allgood Hardware 400x450x1.5mm Satin Stainless Steel Kick Plate. Undrilled.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |

|  |
| --- |
| Total GBP: 1,144.79 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.01.ST05.01 | PM.DR.01.ST10.01 |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 46 -** | **FOH - Leaf & half circulation door - DRT-04a - FWD/15/05/c/FD30 - BLA** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 8.00 ea | SS8066R | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with radius corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 1.00 ea | XX10508FPN | Allgood Hardware intumescent pack for 10508 jamb mounted closer, suitable for timber doors in FD30/60 applications |
| 1.00 ea | SC10508 | Allgood Hardware fully concealed jamb fixed door closer, CE Marked to BS EN: 1154 classification 3-8-3-1-1-3, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 240 minutes on metal doors, satin chrome plated finish (For Fire Pack not supplied order XX10508FPN) |
| 8.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | XX98141S66 | Allgood Hardware, Figure 6, soffit bracket & template, satin stainless steel finish |
| 2.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | SS1761 | Allgood Mode® 700x67x19mm entrance pull handle with bolt through fixings at 600mm centres, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 4.00 ea | SS8449 | Allgood Hardware 76mm circular 'Fire door keep shut' symbol, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, satin stainless steel finish |
| 2.00 ea | SS2301 | Allgood Hardware 38x47mm Heavy Duty Circular Floor Mounted Door Stop, grade 316, 25 year manufacturing warranty, satin stainless steel finish |
| 1.00 ea | ZQ0062637 \* | Allgood Hardware 900x450x1.5mm Satin Stainless Steel Kick Plate. Undrilled.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | ZQ0062638 \* | Allgood Hardware 400x450x1.5mm Satin Stainless Steel Kick Plate. Undrilled.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |

|  |
| --- |
| Total GBP: 1,141.40 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.01.ST.11 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 47 -** | **FOH - Leaf & half access controlled circulation door - DRT-04a - FWD/15/05/c/FD60 - BLA** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 6.00 ea | SS8066R | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with radius corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 1.00 ea | XX10508FPN | Allgood Hardware intumescent pack for 10508 jamb mounted closer, suitable for timber doors in FD30/60 applications |
| 1.00 ea | SC10508 | Allgood Hardware fully concealed jamb fixed door closer, CE Marked to BS EN: 1154 classification 3-8-3-1-1-3, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 240 minutes on metal doors, satin chrome plated finish (For Fire Pack not supplied order XX10508FPN) |
| 12.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 2.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | SS1761 | Allgood Mode® 700x67x19mm entrance pull handle with bolt through fixings at 600mm centres, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 4.00 ea | SS8449 | Allgood Hardware 76mm circular 'Fire door keep shut' symbol, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, satin stainless steel finish |
| 2.00 ea | SS2301 | Allgood Hardware 38x47mm Heavy Duty Circular Floor Mounted Door Stop, grade 316, 25 year manufacturing warranty, satin stainless steel finish |

|  |
| --- |
| Total GBP: 1,017.00 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.00.ST06.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 48 -** | **BOH - Leaf & half circulation door - DRT-05 - BWD/15/05/a/FD60** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 8.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 16.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 2.00 ea | XX97948SS | Allgood Alite® FDKLS 76øx1.2mm 'Fire Door Keep Locked Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | SS48800F | Allgood Hardware 203x19x11mm Lever Action Flush bolt, with coil spring, parallel movement radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48800FP] |
| 1.00 ea | SS48801F | Allgood Hardware 457x19mm Lever Action Flush bolt, with coil spring, parallel movement, radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48801FP] |
| 1.00 ea | SS7051 | Allgood Hardware 63x20x38mm easi-clean socket for wood or stone, grade 316, satin stainless finish |
| 1.00 ea | XX48800FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48800 flush bolts |
| 1.00 ea | XX48801FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48801 flush bolts |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 1.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |
| 1.00 ea | ZQ0062610 \* | 400x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread).  Final Site Size to be confirmed. |

|  |
| --- |
| Total GBP: 655.84 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.00.30A.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| Assumme Doors to have plain meeting stiles.  Slave Leaf width to be confirmed to ensure compatability of door closer and magnetic lock.  May need further discussion. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 50 -** | **FOH - Single access controlled circulation door - DRT-34 - FWD/01/05/c/FD60/AC** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 3.00 ea | SS8066R | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with radius corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 6.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SS1761 | Allgood Mode® 700x67x19mm entrance pull handle with bolt through fixings at 600mm centres, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | XX75574 | Allgood Secure 270x52x28mm surface mounted architectural electromagnet and armature for use on single door applications, 300kg holding force, MBS monitored and dual 12/24 DC voltage with 250ma current draw @ 12 volts and 125ma current draw @ 24 volts, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 60 minutes on metal doors |
| 1.00 ea | XX75574ZLC \* | Allgood Secure Z and L bracket armature assembly complete with architectural cover for use with XX75574 electromagnet. For use on inward opening doors only. |
| 2.00 ea | SS8449 | Allgood Hardware 76mm circular 'Fire door keep shut' symbol, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, satin stainless steel finish |
| 1.00 ea | SS2301 | Allgood Hardware 38x47mm Heavy Duty Circular Floor Mounted Door Stop, grade 316, 25 year manufacturing warranty, satin stainless steel finish |
| 1.00 ea | XX90009 \* | Access control to be supplied by others |

|  |
| --- |
| Total GBP: 492.30 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.01.39.02 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 51 -** | **FOH - Single access controlled circulation door - DRT-34 - FWD/01/05/a/AC** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 3.00 ea | SS8066R | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with radius corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 1.00 ea | SN9133N | Allgood Hardware 280x46x33mm Concealed Overhead Door closer, with finished track & arm for Single Action Doors, adjustable power 2-4, closing force, latch action & cushion stop, Certifire approved CF6022 for use on up to 60 minute timber fire doors & CE Marked to BS EN1154: 3-8-4/2-1-1-3, 10 year manufacturer warranty, SNP finish |
| 1.00 ea | SS1761 | Allgood Mode® 700x67x19mm entrance pull handle with bolt through fixings at 600mm centres, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | SS8451 \* | Allgood Modric® 76ømmx2.5mm 'WC' signage with torx screw fixings, satin stainless steel finish |
| 1.00 ea | SS8454 \* | Allgood Modric® 76ømmx2.5mm 'Staff' signage with torx screw fixings, satin stainless steel finish |
| 1.00 ea | XX75574 | Allgood Secure 270x52x28mm surface mounted architectural electromagnet and armature for use on single door applications, 300kg holding force, MBS monitored and dual 12/24 DC voltage with 250ma current draw @ 12 volts and 125ma current draw @ 24 volts, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 60 minutes on metal doors |
| 1.00 ea | XX75574ZLC \* | Allgood Secure Z and L bracket armature assembly complete with architectural cover for use with XX75574 electromagnet. For use on inward opening doors only. |
| 1.00 ea | SS2301 | Allgood Hardware 38x47mm Heavy Duty Circular Floor Mounted Door Stop, grade 316, 25 year manufacturing warranty, satin stainless steel finish |
| 1.00 ea | XX90009 \* | Access control to be supplied by others |

|  |
| --- |
| Total GBP: 559.41 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.01.40.03 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 52 -** | **FOH - Single access controlled circulation door - DRT-34 - FWD/01/05/c/FD/ - ME Lock** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 3.00 ea | SS8066R | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with radius corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 3.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SN7319AM \* | Allgood Hardware 'A' 60mm (30/30) length Euro Profile Cylinder & turn, independently tested to BS EN 1303:2015 classification 1/6/0/B\*1/0/C/6/D, trademark protection 6 pin cylinder with solid and lateral profile pins, c/w “anti-Bump”, “anti-pick”, “anti-drill” and “anti-pull” protection, 2 keyed, under master key, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors, satin nickel finish |
| 1.00 ea | SS7286F60 | Allgood Hardware 92x60mm backset HL series profile cylinder mortice deadlock case only, single throw 20mm Stainless Steel deadbolt, rounded forend & strike CE Marked to BS EN: 12209 3/X/8/1/0/G/2/B/A/0/0 Certifire approved CF347 for use on 90 minute timber fire doors and up to 240 minutes for metal fire doors, 10 year manufacturing warranty, satin stainless steel finish |
| 1.00 ea | XX7286FP6 | Allgood Hardware intumescent Lock Fire Pack 7286 60mm backset Series |
| 2.00 ea | SS796Q | Allgood Modric® 50x4mm Circular Escutcheon for Euro Profile Cylinder, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and for up to 240 minutes on metal doors, grade 316, 25 year manufacturing warranty, satin stainless steel finish |
| 1.00 ea | SS1763N \* | Allgood Mode® 1300x67x19mm entrance pull handle with bolt through fixings at 1200mm centres for doors 35-54mm thickness, grade 316, satin stainless finish |
| 2.00 ea | SS8449 | Allgood Hardware 76mm circular 'Fire door keep shut' symbol, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, satin stainless steel finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | SS2301 | Allgood Hardware 38x47mm Heavy Duty Circular Floor Mounted Door Stop, grade 316, 25 year manufacturing warranty, satin stainless steel finish |
| 1.00 ea | ZQ0062637 \* | Allgood Hardware 900x450x1.5mm Satin Stainless Steel Kick Plate. Undrilled.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |

|  |
| --- |
| Total GBP: 467.16 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.01.04.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 53 -** | **FOH - Single circulation door - DRT-34 - FWD/01/05/c (a) - Mech HO** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 3.00 ea | SS8066R | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with radius corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 1.00 ea | SN9133N | Allgood Hardware 280x46x33mm Concealed Overhead Door closer, with finished track & arm for Single Action Doors, adjustable power 2-4, closing force, latch action & cushion stop, Certifire approved CF6022 for use on up to 60 minute timber fire doors & CE Marked to BS EN1154: 3-8-4/2-1-1-3, 10 year manufacturer warranty, SNP finish |
| 1.00 ea | ZQ0067743 \* | SS9133NMHO Allgood Hardware 280x46x33mm Concealed Overhead Door closer, with finished track & arm c/w Mechanical Hold Open device \*Not for use on Fire doors\*, for Single Action Doors, adjustable power 2-4, closing force, latch action & cushion stop, CE Marked to BS EN1154: 3-8-4/2-1-1-3, 10 year manufacturer warranty, SNP finish |
| 1.00 ea | SS1761 | Allgood Mode® 700x67x19mm entrance pull handle with bolt through fixings at 600mm centres, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | SS2301 | Allgood Hardware 38x47mm Heavy Duty Circular Floor Mounted Door Stop, grade 316, 25 year manufacturing warranty, satin stainless steel finish |

|  |
| --- |
| Total GBP: 470.80 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.01.15.01 | PM.DR.01.18.01 |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 55 -** | **FOH - Single - Cafe Dry Store / Office - DRT-34 - FWD/01/06/c** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 3.00 ea | SS8066R | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with radius corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 1.00 ea | SN9133N | Allgood Hardware 280x46x33mm Concealed Overhead Door closer, with finished track & arm for Single Action Doors, adjustable power 2-4, closing force, latch action & cushion stop, Certifire approved CF6022 for use on up to 60 minute timber fire doors & CE Marked to BS EN1154: 3-8-4/2-1-1-3, 10 year manufacturer warranty, SNP finish |
| 1.00 ea | SS1763N \* | Allgood Mode® 1300x67x19mm entrance pull handle with bolt through fixings at 1200mm centres for doors 35-54mm thickness, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | SS2301 | Allgood Hardware 38x47mm Heavy Duty Circular Floor Mounted Door Stop, grade 316, 25 year manufacturing warranty, satin stainless steel finish |

|  |
| --- |
| Total GBP: 328.95 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.01.43.01 | PM.DR.01.44.01 |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 56 -** | **FOH - Single - DRT-34 - FWD/01/05/c / ME Lock** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 4.00 ea | SS8066R | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with radius corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 1.00 ea | SN7319AM \* | Allgood Hardware 'A' 60mm (30/30) length Euro Profile Cylinder & turn, independently tested to BS EN 1303:2015 classification 1/6/0/B\*1/0/C/6/D, trademark protection 6 pin cylinder with solid and lateral profile pins, c/w “anti-Bump”, “anti-pick”, “anti-drill” and “anti-pull” protection, 2 keyed, under master key, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors, satin nickel finish |
| 1.00 ea | SS7286F60 | Allgood Hardware 92x60mm backset HL series profile cylinder mortice deadlock case only, single throw 20mm Stainless Steel deadbolt, rounded forend & strike CE Marked to BS EN: 12209 3/X/8/1/0/G/2/B/A/0/0 Certifire approved CF347 for use on 90 minute timber fire doors and up to 240 minutes for metal fire doors, 10 year manufacturing warranty, satin stainless steel finish |
| 2.00 ea | SS796Q | Allgood Modric® 50x4mm Circular Escutcheon for Euro Profile Cylinder, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and for up to 240 minutes on metal doors, grade 316, 25 year manufacturing warranty, satin stainless steel finish |
| 1.00 ea | SS1763N \* | Allgood Mode® 1300x67x19mm entrance pull handle with bolt through fixings at 1200mm centres for doors 35-54mm thickness, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | SS2301 | Allgood Hardware 38x47mm Heavy Duty Circular Floor Mounted Door Stop, grade 316, 25 year manufacturing warranty, satin stainless steel finish |

|  |
| --- |
| Total GBP: 306.84 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.01.LT3.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 57 -** | **FOH - Single lockable circulation door - DRT-34 - FWD/01/06/c/FD60 (a)** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 3.00 ea | SS8066R | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with radius corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 6.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SS1761 | Allgood Mode® 700x67x19mm entrance pull handle with bolt through fixings at 600mm centres, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | SS8449 | Allgood Hardware 76mm circular 'Fire door keep shut' symbol, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, satin stainless steel finish |
| 1.00 ea | SS2301 | Allgood Hardware 38x47mm Heavy Duty Circular Floor Mounted Door Stop, grade 316, 25 year manufacturing warranty, satin stainless steel finish |

|  |
| --- |
| Total GBP: 262.95 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.01.34.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| Is locking required? |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 59 -** | **FOH - Leaf & half lockable circulation door - DRT-35 - FWD/15/06/c** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 6.00 ea | SS8066R | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with radius corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 1.00 ea | SN9133N | Allgood Hardware 280x46x33mm Concealed Overhead Door closer, with finished track & arm for Single Action Doors, adjustable power 2-4, closing force, latch action & cushion stop, Certifire approved CF6022 for use on up to 60 minute timber fire doors & CE Marked to BS EN1154: 3-8-4/2-1-1-3, 10 year manufacturer warranty, SNP finish |
| 1.00 ea | SS1763N \* | Allgood Mode® 1300x67x19mm entrance pull handle with bolt through fixings at 1200mm centres for doors 35-54mm thickness, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | SS48800F | Allgood Hardware 203x19x11mm Lever Action Flush bolt, with coil spring, parallel movement radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48800FP] |
| 1.00 ea | SS7051 | Allgood Hardware 63x20x38mm easi-clean socket for wood or stone, grade 316, satin stainless finish |

|  |
| --- |
| Total GBP: 393.25 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.01.46B.02 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| Assume door leaves to have plain meeting stiles.  Slave leaf width to be confirmed to ensure compatability of door closer. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 60 -** | **FOH - Leaf & half lockable circulation door - DRT-35 - FWD/15/06/c/FD60/EHO** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 6.00 ea | SS8066R | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with radius corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 1.00 ea | XX9133FPNE \* | Allgood Hardware Size 2-4 Concealed Emag Cam Closer Intumescent Pack for use on up to 60 minute timber fire doors to suit 9133NE |
| 1.00 ea | SN9133NE \* | Allgood Hardware 280x46x33mm Concealed Overhead Electrical Hold-open Door Closer, complete with finished track and arm for Single Action Doors, adjustable power '3-4', closing force, latch action, Certifire approved CF6022 & CE Marked to BS EN 1155: 3-8-4/3-1-1-3, 10 year manufacturer warranty, SNP finish |
| 12.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | SS1763N \* | Allgood Mode® 1300x67x19mm entrance pull handle with bolt through fixings at 1200mm centres for doors 35-54mm thickness, grade 316, satin stainless finish |
| 2.00 ea | SS8447 | Allgood Hardware 76mm circular 'Automatic fire door keep clear' symbol, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, satin stainless steel finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | SS48800F | Allgood Hardware 203x19x11mm Lever Action Flush bolt, with coil spring, parallel movement radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48800FP] |
| 1.00 ea | XX90010 \* | See Remarks |
| 2.00 ea | XX48800FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48800 flush bolts |
| 1.00 ea | SS7051 | Allgood Hardware 63x20x38mm easi-clean socket for wood or stone, grade 316, satin stainless finish |
| 2.00 ea | SS8448 | Allgood Hardware 76mm circular 'Fire door keep locked' symbol, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, satin stainless steel finish |
| 1.00 ea | SS2301 | Allgood Hardware 38x47mm Heavy Duty Circular Floor Mounted Door Stop, grade 316, 25 year manufacturing warranty, satin stainless steel finish |

|  |
| --- |
| Total GBP: 694.91 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.01.46A.02 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| PSU in sundries set. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 61 -** | **FOH - Leaf & half access controlled circulation door - DRT-35 - FWD/15/06/d** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 6.00 ea | SS8066R | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with radius corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 1.00 ea | SN9133N | Allgood Hardware 280x46x33mm Concealed Overhead Door closer, with finished track & arm for Single Action Doors, adjustable power 2-4, closing force, latch action & cushion stop, Certifire approved CF6022 for use on up to 60 minute timber fire doors & CE Marked to BS EN1154: 3-8-4/2-1-1-3, 10 year manufacturer warranty, SNP finish |
| 1.00 ea | SS1763N \* | Allgood Mode® 1300x67x19mm entrance pull handle with bolt through fixings at 1200mm centres for doors 35-54mm thickness, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | SS48800F | Allgood Hardware 203x19x11mm Lever Action Flush bolt, with coil spring, parallel movement radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48800FP] |
| 1.00 ea | SS7051 | Allgood Hardware 63x20x38mm easi-clean socket for wood or stone, grade 316, satin stainless finish |
| 1.00 ea | SS2301 | Allgood Hardware 38x47mm Heavy Duty Circular Floor Mounted Door Stop, grade 316, 25 year manufacturing warranty, satin stainless steel finish |
| 1.00 ea | XX90009 \* | Access control to be supplied by others |

|  |
| --- |
| Total GBP: 407.42 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.01.39.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| Assumme Doors to have plain meeting stiles.  Slave Leaf width to be confirmed to ensure compatability of door closer and magnetic lock.  May need further discussion. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 62 -** | **FOH - Leaf & half access controlled circulation door - DRT-35 - FWD/15/06/c/FD60/AC (a)** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 6.00 ea | SS8066R | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with radius corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 1.00 ea | SN9133N | Allgood Hardware 280x46x33mm Concealed Overhead Door closer, with finished track & arm for Single Action Doors, adjustable power 2-4, closing force, latch action & cushion stop, Certifire approved CF6022 for use on up to 60 minute timber fire doors & CE Marked to BS EN1154: 3-8-4/2-1-1-3, 10 year manufacturer warranty, SNP finish |
| 12.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX9133FPN \* | Allgood Hardware Size 2-4 Concealed Cam Closer Intumescent Pack for use on up to 60 minute timber fire doors to suit 9133N |
| 1.00 ea | SS1763N \* | Allgood Mode® 1300x67x19mm entrance pull handle with bolt through fixings at 1200mm centres for doors 35-54mm thickness, grade 316, satin stainless finish |
| 2.00 ea | SS8448 | Allgood Hardware 76mm circular 'Fire door keep locked' symbol, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, satin stainless steel finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | SS48800F | Allgood Hardware 203x19x11mm Lever Action Flush bolt, with coil spring, parallel movement radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48800FP] |
| 1.00 ea | SS7051 | Allgood Hardware 63x20x38mm easi-clean socket for wood or stone, grade 316, satin stainless finish |
| 2.00 ea | XX48800FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48800 flush bolts |
| 2.00 ea | SS8449 | Allgood Hardware 76mm circular 'Fire door keep shut' symbol, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, satin stainless steel finish |
| 1.00 ea | XX75574 | Allgood Secure 270x52x28mm surface mounted architectural electromagnet and armature for use on single door applications, 300kg holding force, MBS monitored and dual 12/24 DC voltage with 250ma current draw @ 12 volts and 125ma current draw @ 24 volts, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 60 minutes on metal doors |
| 1.00 ea | SS2301 | Allgood Hardware 38x47mm Heavy Duty Circular Floor Mounted Door Stop, grade 316, 25 year manufacturing warranty, satin stainless steel finish |
| 1.00 ea | XX90009 \* | Access control to be supplied by others |

|  |
| --- |
| Total GBP: 633.31 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.01.41B.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| Assumme Doors to have plain meeting stiles.  Slave Leaf width to be confirmed to ensure compatability of door closer and magnetic lock.  May need further discussion. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 63 -** | **FOH - Leaf & half circulation door - DRT-37 - FWD/15/05/c/ - Mech HO** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 6.00 ea | SS8066R | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with radius corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 1.00 ea | ZQ0062720 \* | XX98141S6/HO-Allgood hardware surface mounted overhead door closer with mechanical hold open arm, figure 1, adjustable closing speed, power size 2-5, Universal fixings for timber and metal doors, satin stainless steel finish NOT SUITABLE FOR FIRE DOORS |
| 1.00 ea | SS1763N \* | Allgood Mode® 1300x67x19mm entrance pull handle with bolt through fixings at 1200mm centres for doors 35-54mm thickness, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | SS48800F | Allgood Hardware 203x19x11mm Lever Action Flush bolt, with coil spring, parallel movement radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48800FP] |
| 1.00 ea | SS7051 | Allgood Hardware 63x20x38mm easi-clean socket for wood or stone, grade 316, satin stainless finish |
| 1.00 ea | SS2301 | Allgood Hardware 38x47mm Heavy Duty Circular Floor Mounted Door Stop, grade 316, 25 year manufacturing warranty, satin stainless steel finish |
| 2.00 ea | ZQ0062599 \* | Allgood Hardware 55x400x1.5mm Satin Stainless Steel Frame Protection Plate. Undrilled - SELF ADHESIVE BY OTHERS  NOMINAL SIZE ONLY - EXACT SIZES TBC FROM SITE |
| 1.00 ea | ZQ0062637 \* | Allgood Hardware 900x450x1.5mm Satin Stainless Steel Kick Plate. Undrilled.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | ZQ0062638 \* | Allgood Hardware 400x450x1.5mm Satin Stainless Steel Kick Plate. Undrilled.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |

|  |
| --- |
| Total GBP: 494.73 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.01.14.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| Provisional specification subject to approval by door manufacturer. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 64 -** | **FOH - Single sliding door - DRT-44 - FWD/01/05/SD** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 1.00 ea | XX90005 \* | Sliding door gear to be supplied by others |
| 1.00 ea | ZQ0035590 \* | SS7519FN Allgood Hardware 76x58mm backset clawbolt cubicle mortice deadlock with 8mm follower. Radius Forend and strike. |
| 2.00 ea | SS6260 | Allgood Hardware 152x76x22mm flush pull handle for concealed screw fixing, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors, suitable for use on sliding & hinged doors, satin stainless steel finish [For Fire Pack Order XX6250FP] |
| 1.00 ea | SS771Q2530 | Allgood Modric® 50mm dia x 4mm rose and disabled WC turn for bathroom locks, complete with external release/indicator, 5-8mm spindle, 38mm centres with 90 degrees turn action, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 60 minute timber doors, grade 316, 25 year manufacturing warranty, satin stainless steel finish |
| 1.00 ea | XX90008 \* | Signage to be supplied by others |
| 1.00 ea | XX90015 \* | Remainder to be supplied by others |

|  |
| --- |
| Total GBP: 139.23 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.00.58.01 | PM.DR.00.58.02 | PM.DR.00.58.03 |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| All sliding door gear by others. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 65 -** | **FOH - Single lockable circulation door - DRT-34 - FWD/01/06/c/FD60/AC** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 3.00 ea | SS8066R | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with radius corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 6.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SS1761 | Allgood Mode® 700x67x19mm entrance pull handle with bolt through fixings at 600mm centres, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | SS8449 | Allgood Hardware 76mm circular 'Fire door keep shut' symbol, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, satin stainless steel finish |
| 1.00 ea | SS2301 | Allgood Hardware 38x47mm Heavy Duty Circular Floor Mounted Door Stop, grade 316, 25 year manufacturing warranty, satin stainless steel finish |
| 1.00 ea | XX75574 | Allgood Secure 270x52x28mm surface mounted architectural electromagnet and armature for use on single door applications, 300kg holding force, MBS monitored and dual 12/24 DC voltage with 250ma current draw @ 12 volts and 125ma current draw @ 24 volts, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 60 minutes on metal doors |
| 1.00 ea | XX75574ZLC \* | Allgood Secure Z and L bracket armature assembly complete with architectural cover for use with XX75574 electromagnet. For use on inward opening doors only. |
| 1.00 ea | XX90009 \* | Access control to be supplied by others |

|  |
| --- |
| Total GBP: 492.30 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.01.ST12.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 66 -** | **BOH - Leaf & half circulation door - DRT-04 - BWD/15/05/a (a)/ FD30 - BLA** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 8.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 1.00 ea | XX10508FPN | Allgood Hardware intumescent pack for 10508 jamb mounted closer, suitable for timber doors in FD30/60 applications |
| 8.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | SC10508 | Allgood Hardware fully concealed jamb fixed door closer, CE Marked to BS EN: 1154 classification 3-8-3-1-1-3, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 240 minutes on metal doors, satin chrome plated finish (For Fire Pack not supplied order XX10508FPN) |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 2.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 2.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 4.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 2.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 1.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |
| 1.00 ea | ZQ0062610 \* | 400x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread).  Final Site Size to be confirmed. |

|  |
| --- |
| Total GBP: 1,252.01 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.ST05.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| Assumme Doors to have plain meeting stiles.  Slave Leaf width to be confirmed to ensure compatability of door closer.  May need further discussion. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 67 -** | **FOH - Single circulation door - DRT-34 - FWD/01/05/c (KP) - nds** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 3.00 ea | SS8066R | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with radius corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 1.00 ea | SN9133N | Allgood Hardware 280x46x33mm Concealed Overhead Door closer, with finished track & arm for Single Action Doors, adjustable power 2-4, closing force, latch action & cushion stop, Certifire approved CF6022 for use on up to 60 minute timber fire doors & CE Marked to BS EN1154: 3-8-4/2-1-1-3, 10 year manufacturer warranty, SNP finish |
| 1.00 ea | SS1761 | Allgood Mode® 700x67x19mm entrance pull handle with bolt through fixings at 600mm centres, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | ZQ0062637 \* | Allgood Hardware 900x450x1.5mm Satin Stainless Steel Kick Plate. Undrilled.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |

|  |
| --- |
| Total GBP: 361.10 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.01.55.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 70 -** | **BOH - Single Unisex/Gender Neutral entrance door - DRT-02a - BWD/01/05/a/U/FD30 - 1M High P/P** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 3.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 3.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069803 \* | Allgood Hardware 1000x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixing -  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | XX97934SS | Allgood Alite® 76øx1.2mm 'Unisex' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |

|  |
| --- |
| Total GBP: 195.42 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.28.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| Listed as Door type DRT-02a with a Laminate finish though Door Type/Material is listed as Metal.  Pictogram subject to approval.  Requirements if differ from scheduled hardware set to be advised prior to order. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 71 -** | **BOH - Leaf & half access controlled circulation door - DRT-04 - BWD/15/05/a/EHO/FD60/AC/BLA - (Frame Protection) - BLA** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 8.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 2.00 ea | SS9409 | Allgood Hardware 86x86mm Wall Mounted Fire Door Holder, 24vDC, satin stainless steel finish |
| 2.00 ea | SS9410 | Allgood Hardware surface mounted bracket for 9409 door holder, satin stainless steel finish |
| 16.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SC10508 | Allgood Hardware fully concealed jamb fixed door closer, CE Marked to BS EN: 1154 classification 3-8-3-1-1-3, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 240 minutes on metal doors, satin chrome plated finish (For Fire Pack not supplied order XX10508FPN) |
| 1.00 ea | XX10508FPN | Allgood Hardware intumescent pack for 10508 jamb mounted closer, suitable for timber doors in FD30/60 applications |
| 1.00 ea | SS1771SFF \* | Allgood Mode® 619x65x19mm mitred pull handle with concealed face fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 2.00 ea | XX30057 | Allgood Hardware 600x100mm PVC Sign 50mm letters 'push bar to open' (No Screws Supplied) |
| 4.00 ea | XX97947SS | Allgood Alite® ADFKC 76øx1.2mm 'Automatic Fire Door Keep Clear' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 4.00 ea | XX97950SS \* | Allgood Alite® FEKC 76øx1.2mm 'Fire Exit Keep Clear' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | XX9320S | Allgood Hardware touchbar 3 Point vertical rod panic bolt, suitable for wood, steel and aluminium doors, 840mm wide x 2650mm high, Certifire approved CF5516, CE/UKCA marked to EN1125 3-7-7-B-1-4-2-2-B-A, satin simulated stainless steel finish |
| 1.00 ea | XX9329s \* | Allgood Hardware "Motorised" Touchbar 3 Point vertical rod panic bolt, suitable for wood, steel and aluminium doors, 840mm wide x 2650mm high, Certifire approved CF5516, CE/UKCA marked to EN1125 3-7-7-B-1-4-2-2-B-A, satin simulated stainless steel finish |
| 2.00 ea | ZQ0062599 \* | Allgood Hardware 55x400x1.5mm Satin Stainless Steel Frame Protection Plate. Undrilled - SELF ADHESIVE BY OTHERS  NOMINAL SIZE ONLY - EXACT SIZES TBC FROM SITE |
| 2.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 1.00 ea | XX90010 \* | See Remarks |
| 2.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |
| 1.00 ea | ZQ0062610 \* | 400x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread).  Final Site Size to be confirmed. |
| 1.00 ea | XX90009 \* | Access control to be supplied by others |

|  |
| --- |
| Total GBP: 2,796.55 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.10.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| Assumme Doors to have plain meeting stiles.  PSU in sundries set  Jamb mounted closer required for your half leaf as the leaf is less than 400mm wide. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 72 -** | **BOH - Leaf & half access controlled circulation door - DRT-04 - BWD/15/05/a/FD60/AC/Fig6** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 8.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 16.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S66 | Allgood Hardware, Figure 6, soffit bracket & template, satin stainless steel finish |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | XX97948SS | Allgood Alite® FDKLS 76øx1.2mm 'Fire Door Keep Locked Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | SS48800F | Allgood Hardware 203x19x11mm Lever Action Flush bolt, with coil spring, parallel movement radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48800FP] |
| 1.00 ea | SS48801F | Allgood Hardware 457x19mm Lever Action Flush bolt, with coil spring, parallel movement, radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48801FP] |
| 1.00 ea | SS7051 | Allgood Hardware 63x20x38mm easi-clean socket for wood or stone, grade 316, satin stainless finish |
| 1.00 ea | XX48800FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48800 flush bolts |
| 1.00 ea | XX48801FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48801 flush bolts |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | XX75574 | Allgood Secure 270x52x28mm surface mounted architectural electromagnet and armature for use on single door applications, 300kg holding force, MBS monitored and dual 12/24 DC voltage with 250ma current draw @ 12 volts and 125ma current draw @ 24 volts, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 60 minutes on metal doors |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 1.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |
| 1.00 ea | ZQ0062610 \* | 400x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread).  Final Site Size to be confirmed. |
| 1.00 ea | XX90009 \* | Access control to be supplied by others |

|  |
| --- |
| Total GBP: 803.88 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.31.01 | PM.DR.BM.19.01 |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| Assumme Doors to have plain meeting stiles. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 73 -** | **BOH - Leaf & half access controlled circulation door - DRT-04 - BWD/15/05/a/FD30/AC - BLA** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 8.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 1.00 ea | XX10508FPN | Allgood Hardware intumescent pack for 10508 jamb mounted closer, suitable for timber doors in FD30/60 applications |
| 1.00 ea | SC10508 | Allgood Hardware fully concealed jamb fixed door closer, CE Marked to BS EN: 1154 classification 3-8-3-1-1-3, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 240 minutes on metal doors, satin chrome plated finish (For Fire Pack not supplied order XX10508FPN) |
| 8.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | XX98141S66 | Allgood Hardware, Figure 6, soffit bracket & template, satin stainless steel finish |
| 1.00 ea | SS1771SFF \* | Allgood Mode® 619x65x19mm mitred pull handle with concealed face fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 2.00 ea | XX30057 | Allgood Hardware 600x100mm PVC Sign 50mm letters 'push bar to open' (No Screws Supplied) |
| 4.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 4.00 ea | XX97950SS \* | Allgood Alite® FEKC 76øx1.2mm 'Fire Exit Keep Clear' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | XX9320S | Allgood Hardware touchbar 3 Point vertical rod panic bolt, suitable for wood, steel and aluminium doors, 840mm wide x 2650mm high, Certifire approved CF5516, CE/UKCA marked to EN1125 3-7-7-B-1-4-2-2-B-A, satin simulated stainless steel finish |
| 1.00 ea | XX9329s \* | Allgood Hardware "Motorised" Touchbar 3 Point vertical rod panic bolt, suitable for wood, steel and aluminium doors, 840mm wide x 2650mm high, Certifire approved CF5516, CE/UKCA marked to EN1125 3-7-7-B-1-4-2-2-B-A, satin simulated stainless steel finish |
| 2.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 1.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |
| 1.00 ea | ZQ0062610 \* | 400x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread).  Final Site Size to be confirmed. |
| 1.00 ea | XX90009 \* | Access control to be supplied by others |

|  |
| --- |
| Total GBP: 2,322.40 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.ST11.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| Assumme Doors to have plain meeting stiles. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 74 -** | **BOH - Leaf & half access controlled circulation door - DRT-04 - BWD/15/05/a/FD30/AC/ - Fig 6 - BLA** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 8.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 1.00 ea | XX10508FPN | Allgood Hardware intumescent pack for 10508 jamb mounted closer, suitable for timber doors in FD30/60 applications |
| 1.00 ea | SC10508 | Allgood Hardware fully concealed jamb fixed door closer, CE Marked to BS EN: 1154 classification 3-8-3-1-1-3, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 240 minutes on metal doors, satin chrome plated finish (For Fire Pack not supplied order XX10508FPN) |
| 8.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S66 | Allgood Hardware, Figure 6, soffit bracket & template, satin stainless steel finish |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SS1771SFF \* | Allgood Mode® 619x65x19mm mitred pull handle with concealed face fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 2.00 ea | XX30057 | Allgood Hardware 600x100mm PVC Sign 50mm letters 'push bar to open' (No Screws Supplied) |
| 4.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 4.00 ea | XX97950SS \* | Allgood Alite® FEKC 76øx1.2mm 'Fire Exit Keep Clear' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | XX9320S | Allgood Hardware touchbar 3 Point vertical rod panic bolt, suitable for wood, steel and aluminium doors, 840mm wide x 2650mm high, Certifire approved CF5516, CE/UKCA marked to EN1125 3-7-7-B-1-4-2-2-B-A, satin simulated stainless steel finish |
| 1.00 ea | XX9329s \* | Allgood Hardware "Motorised" Touchbar 3 Point vertical rod panic bolt, suitable for wood, steel and aluminium doors, 840mm wide x 2650mm high, Certifire approved CF5516, CE/UKCA marked to EN1125 3-7-7-B-1-4-2-2-B-A, satin simulated stainless steel finish |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 1.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |
| 1.00 ea | ZQ0062610 \* | 400x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread).  Final Site Size to be confirmed. |
| 1.00 ea | XX90009 \* | Access control to be supplied by others |

|  |
| --- |
| Total GBP: 2,316.83 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.ST10.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| Assumme Doors to have plain meeting stiles.  Jamb mounted closer required for your half leaf as the leaf is less than 400mm wide. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 75 -** | **BOH - Leaf & half access controlled circulation door - DRT-04 - BWD/15/05/a/FD60/AC/Fig6 - BLA** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 8.00 ea | SS8066R | Allgood Hardware 100x75x3mm, Grade 14, Triple Knuckle Concealed Bearing Button Tipped Hinges, with radius corners, N° 10 woodscrews, independently tested to 1 million cycles, CE marked to EN 1935 classification 4-7-7-1-1-4-0-14, suitable for doors up to 160kg, Certifire approved CF5689 for use on timber fire doors up to 120 minutes and metal fire doors up to 240 minutes, 25 year manufacturer warranty, grade 304, satin stainless steel finish |
| 1.00 ea | XX10508FPN | Allgood Hardware intumescent pack for 10508 jamb mounted closer, suitable for timber doors in FD30/60 applications |
| 1.00 ea | SC10508 | Allgood Hardware fully concealed jamb fixed door closer, CE Marked to BS EN: 1154 classification 3-8-3-1-1-3, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 240 minutes on metal doors, satin chrome plated finish (For Fire Pack not supplied order XX10508FPN) |
| 16.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | XX98141S66 | Allgood Hardware, Figure 6, soffit bracket & template, satin stainless steel finish |
| 4.00 ea | SS8449 | Allgood Hardware 76mm circular 'Fire door keep shut' symbol, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, satin stainless steel finish |
| 2.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | SS2301 | Allgood Hardware 38x47mm Heavy Duty Circular Floor Mounted Door Stop, grade 316, 25 year manufacturing warranty, satin stainless steel finish |
| 1.00 ea | XX75574D \* | Allgood Secure 520x52x28mm Surface Mounted Architectural Electromagnet and Armature, for use on double door applications, 300kg holding force (on each door leaf), MBS monitored and dual 12/24 DC voltage, with 500ma current draw @ 12 volts and 250ma current draw @ 24 volts, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 60 minutes on metal doors |
| 1.00 ea | XX90009 \* | Access control to be supplied by others |
| 1.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |
| 1.00 ea | ZQ0062610 \* | 400x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread).  Final Site Size to be confirmed. |

|  |
| --- |
| Total GBP: 1,670.76 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.ST06.02 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| Assume doors to have plain meeting stiles.  Jamb mounted closer required for your half leaf as the leaf is less than 400mm wide. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 76 -** | **BOH - Leaf & half circulation door - DRT-04 - BWD/15/05/a/CL-EQ/FD30** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 1.00 ea | SS7636F \* | Spare Radius Strike Plate for Deadlock New 76 Series SS7686FS60 |
| 8.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 8.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SN7319AM \* | Allgood Hardware 'A' 60mm (30/30) length Euro Profile Cylinder & turn, independently tested to BS EN 1303:2015 classification 1/6/0/B\*1/0/C/6/D, trademark protection 6 pin cylinder with solid and lateral profile pins, c/w “anti-Bump”, “anti-pick”, “anti-drill” and “anti-pull” protection, 2 keyed, under master key, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors, satin nickel finish |
| 1.00 ea | SS7686FN60 | Allgood Hardware 93x60mm backset profile cylinder mortice deadlock case only, double throw 20mm deadbolt, CE Marked to BS EN 12209 3/X/8/1/0/G/2/B/C/0/0, Certifire approved CF5899 for use up to 120 minutes on timber fire doors and 240 minute metal fire doors, radius forend & square strike, satin stainless steel finish |
| 1.00 ea | XX7679FP1 | Allgood Hardware intumescent Pack for 76 Series 60mm Backset TFD30, TFD60 |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 2.00 ea | XX97876SS | Allgood Alite® Cylinder Rose, 50mm diameter concealed with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 60 minute timber doors, satin stainless steel finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | XX97948SS | Allgood Alite® FDKLS 76øx1.2mm 'Fire Door Keep Locked Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | XX97955SS | Allgood Alite® 76øx1.2mm 'Cleaners' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | SS48800F | Allgood Hardware 203x19x11mm Lever Action Flush bolt, with coil spring, parallel movement radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48800FP] |
| 1.00 ea | SS48801F | Allgood Hardware 457x19mm Lever Action Flush bolt, with coil spring, parallel movement, radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48801FP] |
| 1.00 ea | XX48800FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48800 flush bolts |
| 1.00 ea | XX48801FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48801 flush bolts |
| 1.00 ea | SS7051 | Allgood Hardware 63x20x38mm easi-clean socket for wood or stone, grade 316, satin stainless finish |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 1.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |
| 1.00 ea | ZQ0062610 \* | 400x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread).  Final Site Size to be confirmed. |

|  |
| --- |
| Total GBP: 734.79 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.40.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 79 -** | **BOH - Single cleaners cupboard - DRT-02a - FWD/01/07/CL/FD60 - PH** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 1.00 ea | SS7636F \* | Spare Radius Strike Plate for Deadlock New 76 Series SS7686FS60 |
| 4.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 8.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SN7319AM \* | Allgood Hardware 'A' 60mm (30/30) length Euro Profile Cylinder & turn, independently tested to BS EN 1303:2015 classification 1/6/0/B\*1/0/C/6/D, trademark protection 6 pin cylinder with solid and lateral profile pins, c/w “anti-Bump”, “anti-pick”, “anti-drill” and “anti-pull” protection, 2 keyed, under master key, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors, satin nickel finish |
| 1.00 ea | SS7686FN60 | Allgood Hardware 93x60mm backset profile cylinder mortice deadlock case only, double throw 20mm deadbolt, CE Marked to BS EN 12209 3/X/8/1/0/G/2/B/C/0/0, Certifire approved CF5899 for use up to 120 minutes on timber fire doors and 240 minute metal fire doors, radius forend & square strike, satin stainless steel finish |
| 1.00 ea | XX7679FP1 | Allgood Hardware intumescent Pack for 76 Series 60mm Backset TFD30, TFD60 |
| 2.00 ea | XX97876SS | Allgood Alite® Cylinder Rose, 50mm diameter concealed with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 60 minute timber doors, satin stainless steel finish |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | XX97955SS | Allgood Alite® 76øx1.2mm 'Cleaners' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |

|  |
| --- |
| Total GBP: 297.97 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.00.44B.01 | PM.DR.00.61.01 |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 80 -** | **BOH - Single access locked door w/levers - DRT-02 - BWD/01/09/a/FD60a** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 1.00 ea | SS7631F \* | Spare Radius Strike Plate for Bathroom/Sashlock New 76 Series SS7608FS60/SS7679FS60 |
| 4.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 8.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | SN7319BM \* | Allgood Hardware 'B' 70mm (35/35) length Euro Profile Cylinder & turn, independently tested to BS EN 1303:2015 classification 1/6/0/B\*1/0/C/6/D, trademark protection 6 pin cylinder with solid and lateral profile pins, c/w “anti-Bump”, “anti-pick”, “anti-drill” and “anti-pull” protection, 2 keyed, under master key, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors, satin nickel plated finish |
| 1.00 ea | SS7679FN60 | Allgood Hardware 93x60mm backset profile cylinder mortice lock case only, heavy sprung for levers, double throw deadbolt, CE Marked to BS EN 12209 3/X/8/1/0/G/2/B/C/2/0, Certifire approved CF5899 for use up to 120 minutes on timber fire doors and 240 minute metal fire doors, radius forend & square strike, satin stainless steel finish |
| 1.00 ea | XX7679FP1 | Allgood Hardware intumescent Pack for 76 Series 60mm Backset TFD30, TFD60 |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 pr | XX97423SSN | Allgood Alite® 127 x 64mm x 19mmØ Straight lever handles, on Quadaxial® 50Ø x 4mm concealed fixing roses (tested to 1 million cycles), independently tested to BS EN 1906 4/7/-/1/0/3/0/U, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, suitable for doors 35-54mm, grade 304, satin stainless steel finish |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 2.00 ea | XX97876SS | Allgood Alite® Cylinder Rose, 50mm diameter concealed with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 60 minute timber doors, satin stainless steel finish |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |

|  |
| --- |
| Total GBP: 464.53 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.PL10.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 81 -** | **BOH - Single circulation door - DRT-02 - BWD/01/05/a/FD60a** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 4.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 8.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |

|  |
| --- |
| Total GBP: 431.64 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.04.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 82 -** | **BOH - Single circulation door - DRT-02 - BWD/01/05/a/FD30a - 1M High P/P** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 4.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 4.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069803 \* | Allgood Hardware 1000x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixing -  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |

|  |
| --- |
| Total GBP: 419.18 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.23.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 83 -** | **BOH - Single lockable door w/levers - DRT-02 - BWD/01/09/a/FD60b - Fig 6** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 1.00 ea | SS7631F \* | Spare Radius Strike Plate for Bathroom/Sashlock New 76 Series SS7608FS60/SS7679FS60 |
| 4.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 8.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | XX98141S66 | Allgood Hardware, Figure 6, soffit bracket & template, satin stainless steel finish |
| 1.00 ea | SN7319AM \* | Allgood Hardware 'A' 60mm (30/30) length Euro Profile Cylinder & turn, independently tested to BS EN 1303:2015 classification 1/6/0/B\*1/0/C/6/D, trademark protection 6 pin cylinder with solid and lateral profile pins, c/w “anti-Bump”, “anti-pick”, “anti-drill” and “anti-pull” protection, 2 keyed, under master key, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors, satin nickel finish |
| 1.00 ea | SS7679FN60 | Allgood Hardware 93x60mm backset profile cylinder mortice lock case only, heavy sprung for levers, double throw deadbolt, CE Marked to BS EN 12209 3/X/8/1/0/G/2/B/C/2/0, Certifire approved CF5899 for use up to 120 minutes on timber fire doors and 240 minute metal fire doors, radius forend & square strike, satin stainless steel finish |
| 1.00 ea | XX7679FP1 | Allgood Hardware intumescent Pack for 76 Series 60mm Backset TFD30, TFD60 |
| 1.00 pr | XX97423SSN | Allgood Alite® 127 x 64mm x 19mmØ Straight lever handles, on Quadaxial® 50Ø x 4mm concealed fixing roses (tested to 1 million cycles), independently tested to BS EN 1906 4/7/-/1/0/3/0/U, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, suitable for doors 35-54mm, grade 304, satin stainless steel finish |
| 2.00 ea | XX97876SS | Allgood Alite® Cylinder Rose, 50mm diameter concealed with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 60 minute timber doors, satin stainless steel finish |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |

|  |
| --- |
| Total GBP: 243.05 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.30.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 84 -** | **BOH - Single lockable door w/levers - DRT-02 - BWD/01/09/a/FD60c - Fig 1 / nds** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 1.00 ea | SS7631F \* | Spare Radius Strike Plate for Bathroom/Sashlock New 76 Series SS7608FS60/SS7679FS60 |
| 4.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 8.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SN7319AM \* | Allgood Hardware 'A' 60mm (30/30) length Euro Profile Cylinder & turn, independently tested to BS EN 1303:2015 classification 1/6/0/B\*1/0/C/6/D, trademark protection 6 pin cylinder with solid and lateral profile pins, c/w “anti-Bump”, “anti-pick”, “anti-drill” and “anti-pull” protection, 2 keyed, under master key, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors, satin nickel finish |
| 1.00 ea | SS7679FN60 | Allgood Hardware 93x60mm backset profile cylinder mortice lock case only, heavy sprung for levers, double throw deadbolt, CE Marked to BS EN 12209 3/X/8/1/0/G/2/B/C/2/0, Certifire approved CF5899 for use up to 120 minutes on timber fire doors and 240 minute metal fire doors, radius forend & square strike, satin stainless steel finish |
| 1.00 ea | XX7679FP1 | Allgood Hardware intumescent Pack for 76 Series 60mm Backset TFD30, TFD60 |
| 1.00 pr | XX97423SSN | Allgood Alite® 127 x 64mm x 19mmØ Straight lever handles, on Quadaxial® 50Ø x 4mm concealed fixing roses (tested to 1 million cycles), independently tested to BS EN 1906 4/7/-/1/0/3/0/U, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, suitable for doors 35-54mm, grade 304, satin stainless steel finish |
| 2.00 ea | XX97876SS | Allgood Alite® Cylinder Rose, 50mm diameter concealed with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 60 minute timber doors, satin stainless steel finish |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |

|  |
| --- |
| Total GBP: 453.49 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.PL16.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 85 -** | **BOH - Leaf & half access controlled circulation door - DRT-04 - BWD/15/05/a/FD60a - Fig 1** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 8.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 16.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | XX97948SS | Allgood Alite® FDKLS 76øx1.2mm 'Fire Door Keep Locked Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | SS48800F | Allgood Hardware 203x19x11mm Lever Action Flush bolt, with coil spring, parallel movement radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48800FP] |
| 1.00 ea | SS48801F | Allgood Hardware 457x19mm Lever Action Flush bolt, with coil spring, parallel movement, radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48801FP] |
| 1.00 ea | SS7051 | Allgood Hardware 63x20x38mm easi-clean socket for wood or stone, grade 316, satin stainless finish |
| 1.00 ea | XX48800FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48800 flush bolts |
| 1.00 ea | XX48801FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48801 flush bolts |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 1.00 ea | XX75574 | Allgood Secure 270x52x28mm surface mounted architectural electromagnet and armature for use on single door applications, 300kg holding force, MBS monitored and dual 12/24 DC voltage with 250ma current draw @ 12 volts and 125ma current draw @ 24 volts, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 60 minutes on metal doors |
| 1.00 ea | XX75574ZLC \* | Allgood Secure Z and L bracket armature assembly complete with architectural cover for use with XX75574 electromagnet. For use on inward opening doors only. |
| 1.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |
| 1.00 ea | ZQ0062610 \* | 400x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread).  Final Site Size to be confirmed. |
| 1.00 ea | XX90009 \* | Access control to be supplied by others |

|  |
| --- |
| Total GBP: 885.19 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.07.04 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| Assumme Doors to have plain meeting stiles. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 86 -** | **BOH - Double access controlled circulation door - DRT-01 - BWD/02/05/a/EHO/FD60/AC - 1ds - Frame Protection - BLA** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 8.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 16.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 2.00 ea | XX98141S66 | Allgood Hardware, Figure 6, soffit bracket & template, satin stainless steel finish |
| 2.00 ea | XX98181S6 | Allgood Hardware Surface Mounted Electromagnetic Hold Open Overhead Door Closer, with swing free option, controlled closing, power size 4, universal fixings for timber and metal doors, supplied c/w black power transfer loop, frame mounted connection box and on/off switch, Certifire CF5517 listed to BS EN 1155, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on insulated metal doors, 10 year manufacturer warranty, satin stainless steel finish |
| 2.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 2.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 4.00 ea | XX97947SS | Allgood Alite® ADFKC 76øx1.2mm 'Automatic Fire Door Keep Clear' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 2.00 ea | ZQ0062599 \* | Allgood Hardware 55x400x1.5mm Satin Stainless Steel Frame Protection Plate. Undrilled - SELF ADHESIVE BY OTHERS  NOMINAL SIZE ONLY - EXACT SIZES TBC FROM SITE |
| 1.00 ea | XX75574D \* | Allgood Secure 520x52x28mm Surface Mounted Architectural Electromagnet and Armature, for use on double door applications, 300kg holding force (on each door leaf), MBS monitored and dual 12/24 DC voltage, with 500ma current draw @ 12 volts and 250ma current draw @ 24 volts, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 60 minutes on metal doors |
| 1.00 ea | XX75574DZLC \* | Allgood Secure Z and L bracket armature assembly complete with architectural cover for use with XX75574D electromagnet. For use on inward opening doors only, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 60 minutes on metal doors |
| 2.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |
| 1.00 ea | XX90009 \* | Access control to be supplied by others |

|  |
| --- |
| Total GBP: 1,736.25 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.22.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| We have assumed doors have plain meeting stiles.  Make up of frame protection plate to be confirmed. Offcuts of tread plate to be considered. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 87 -** | **BOH - Double circulation door - DRT-01 - BWD/02/05/a/EHO/FD60/b - (Frame Protection) - BLA** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 8.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 16.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 2.00 ea | XX98141S66 | Allgood Hardware, Figure 6, soffit bracket & template, satin stainless steel finish |
| 2.00 ea | XX98181S6 | Allgood Hardware Surface Mounted Electromagnetic Hold Open Overhead Door Closer, with swing free option, controlled closing, power size 4, universal fixings for timber and metal doors, supplied c/w black power transfer loop, frame mounted connection box and on/off switch, Certifire CF5517 listed to BS EN 1155, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on insulated metal doors, 10 year manufacturer warranty, satin stainless steel finish |
| 2.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 2.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 4.00 ea | XX97947SS | Allgood Alite® ADFKC 76øx1.2mm 'Automatic Fire Door Keep Clear' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 2.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 2.00 ea | ZQ0062599 \* | Allgood Hardware 55x400x1.5mm Satin Stainless Steel Frame Protection Plate. Undrilled - SELF ADHESIVE BY OTHERS  NOMINAL SIZE ONLY - EXACT SIZES TBC FROM SITE |
| 2.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |

|  |
| --- |
| Total GBP: 1,289.46 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.58.03 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| Make up of frame protection plate to be confirmed. Offcuts of tread plate to be considered. |  |  |  |
| We have assumed doors have plain meeting stiles.  PSU in sundries set |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 88 -** | **BOH - Double circulation door - DRT-01 - BWD/02/05/a/FD60/2a - 1ds - Frame Protection** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 8.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 16.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | XX97948SS | Allgood Alite® FDKLS 76øx1.2mm 'Fire Door Keep Locked Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | SS48800F | Allgood Hardware 203x19x11mm Lever Action Flush bolt, with coil spring, parallel movement radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48800FP] |
| 1.00 ea | SS48801F | Allgood Hardware 457x19mm Lever Action Flush bolt, with coil spring, parallel movement, radius ends, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 for use on 30 & 60 minute timber doors, grade 316, satin stainless steel finish [For Fire Pack Order XX48801FP] |
| 1.00 ea | SS7051 | Allgood Hardware 63x20x38mm easi-clean socket for wood or stone, grade 316, satin stainless finish |
| 1.00 ea | XX48800FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48800 flush bolts |
| 1.00 ea | XX48801FP | Allgood Hardware intumescent pack for FD30 & FD60 timber fire doors to suit 48801 flush bolts |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 2.00 ea | ZQ0062599 \* | Allgood Hardware 55x400x1.5mm Satin Stainless Steel Frame Protection Plate. Undrilled - SELF ADHESIVE BY OTHERS  NOMINAL SIZE ONLY - EXACT SIZES TBC FROM SITE |
| 2.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |

|  |
| --- |
| Total GBP: 772.49 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.B1.54.01 | PM.DR.B1.PL03A.02 |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| We have assumed doors have plain meeting stiles. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 89 -** | **BOH - Single circulation door - DRT-02 - BWD/01/05/a/FD60b - Frame Protection** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 4.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 8.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | SS21705 | Allgood Alite® Floor Mounted Door Stop 45x25mm, grade 316, satin stainless steel |
| 1.00 ea | ZQ0062599 \* | Allgood Hardware 55x400x1.5mm Satin Stainless Steel Frame Protection Plate. Undrilled - SELF ADHESIVE BY OTHERS  NOMINAL SIZE ONLY - EXACT SIZES TBC FROM SITE |
| 1.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |

|  |
| --- |
| Total GBP: 443.30 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.BM.01.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| PM.DR.B1.PL21.02 - Components subject to approval by door manufacturer to ensure compliance with security rating. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 90 -** | **BOH - Single circulation door - DRT-02 - BWD/01/05/a/FD60c - nds** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 4.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 8.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |

|  |
| --- |
| Total GBP: 426.07 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.BM.18.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| PM.DR.B1.PL21.02 - Components subject to approval by door manufacturer to ensure compliance with security rating. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 91 -** | **BOH - Single circulation door DRT-02 WD/01/05/FD60 - nds - Fig 6** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 4.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 8.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | XX98141S66 | Allgood Hardware, Figure 6, soffit bracket & template, satin stainless steel finish |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |

|  |
| --- |
| Total GBP: 431.72 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.00.25.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| PM.DR.B1.PL21.02 - Components subject to approval by door manufacturer to ensure compliance with security rating. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 92 -** | **BOH - Single access controlled circulation door - DRT-02 - BWD/01/05/a/FD60/AC- nds** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 4.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 8.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |
| 1.00 ea | XX75574 | Allgood Secure 270x52x28mm surface mounted architectural electromagnet and armature for use on single door applications, 300kg holding force, MBS monitored and dual 12/24 DC voltage with 250ma current draw @ 12 volts and 125ma current draw @ 24 volts, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 60 minutes on metal doors |
| 1.00 ea | XX75574ZLC \* | Allgood Secure Z and L bracket armature assembly complete with architectural cover for use with XX75574 electromagnet. For use on inward opening doors only. |
| 1.00 ea | XX90009 \* | Access control to be supplied by others |

|  |
| --- |
| Total GBP: 655.42 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.BM.04.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Set 93 -** | **BOH - Single access controlled circulation door - DRT-02 - BWD/01/05/a/FD60/AC/f - nds - Frame Protection** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 4.00 ea | SS97501R | Allgood 102x76x3mm Butt Hinges, with radius corners, CE Marked for fire and escape doors to BS EN 1935 classification 4-7-6-1-1-4-0-13, Certifire approved CF749 for use up to 120 minute timber fire doors and 240 minute metal fire doors, subject to regular lubrication to manufacturer's instructions, satin stainless steel finish |
| 8.00 ea | XX8066FP | Allgood Hardware 98x27x1mm intumescent pack to suit 8066 & 97501 butt hinges comprising 2 Blades per pack, 1 pack required per hinge for FD30 / 2 packs per hinge for FD60/FD90/FD120 applications |
| 1.00 ea | XX98141S6 | Allgood hardware surface mounted overhead door closer, figure 1, adjustable closing speed, adjustable backcheck, power size 2-5, Universal fixings for timber and metal doors, CE Marked and Certifire CF641 listed to BS EN 1154 classification 4-8-(2-5)-1-1-3, incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 mins on timber doors and up to 240 mins on metal door, 10 year manufacturer warranty, satin stainless steel finish |
| 1.00 ea | SS1771 | Allgood Mode® 619x65x19mm pull handle with bolt through fixings at 600mm centres for doors 10-55mm thick, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 120 minutes on metal doors, grade 316, satin stainless finish |
| 1.00 ea | ZQ0069564 \* | Allgood Hardware 1200x150x1.5mm Grade 304 Satin Stainless Steel Push Plate. Satin Stainless Steel Finish. Drilled & Countersunk With Torx Screw Fixings.  NOMINAL SIZE ONLY - FINAL SIZES TO BE CONFIRMED |
| 2.00 ea | XX97949SS | Allgood Alite® FDKS 76øx1.2mm 'Fire Door Keep Shut' Symbol Disc, with screw fixings, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 120 minutes on timber doors and 240 minutes on metal doors, grade 430, satin stainless steel finish, Horizontal Grain |
| 1.00 ea | ZQ0062599 \* | Allgood Hardware 55x400x1.5mm Satin Stainless Steel Frame Protection Plate. Undrilled - SELF ADHESIVE BY OTHERS  NOMINAL SIZE ONLY - EXACT SIZES TBC FROM SITE |
| 1.00 ea | ZQ0062609 \* | 900x400x3.0m Stainless Steel Chequer Plate. No Fixings (3mm base 1.5mm tread)  Final Site Size to be confirmed. |
| 1.00 ea | XX75574 | Allgood Secure 270x52x28mm surface mounted architectural electromagnet and armature for use on single door applications, 300kg holding force, MBS monitored and dual 12/24 DC voltage with 250ma current draw @ 12 volts and 125ma current draw @ 24 volts, Incorporated in successful fire tests and assessed to BS EN 1634-1 and BS 476 Pt 22 up to 60 minutes on timber doors and 60 minutes on metal doors |
| 1.00 ea | XX75574ZLC \* | Allgood Secure Z and L bracket armature assembly complete with architectural cover for use with XX75574 electromagnet. For use on inward opening doors only. |
| 1.00 ea | XX90009 \* | Access control to be supplied by others |

|  |
| --- |
| Total GBP: 667.08 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| PM.DR.BM.08.01 |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Sundries -** | **Sundries** |  |  |

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item number** | **Description** |
| 1.00 ea | XX7357AM \* | Allgood Hardware master key |
| 1.00 ea | XX7358AM \* | Allgood Hardware sub master key |
| 3.00 ea | XX79011N1 | Allgood Secure 24 volt DC, 1amp Switch Mode Power supply, box size 235x170x85mm |
| 1.00 ea | XX90010 \* | See Remarks |

|  |
| --- |
| Total GBP: 293.62 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Numbers** |  |  |  |  |  |
|  |  |  |  |  |  |
| misc |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Remarks** |  |  |  |
| Optional sundry item quantities to be confirmed prior to order. |  |  |  |
|  |  |  |  |
| A nominal quantity of certified 24v DC switch mode transformers have been allowed for within our specification. Our calculations are based on 6 devices being powered from 1 single 24v DC transformer. Please note that additional transformers may be required should it not be viable to group and control hold open devices in to groups of 6. Cable distance and volt drop can affect the overall performance of each hold open device. Sensible measures should be taken to reduce volt drop (locate each transformer in close proximity to each door group. Ensure suitable low voltage cable is used. 1no 230V supply feed and 1no fire alarm interface will be required at each transformer location. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Page** | **Hardware Set** | **Quantity** | **Unit Price** | **Total Price** |
|  |  |  |  |  |
| 4 | Set 01 | 3.00 | 978.52 | 2,935.56 |
| 6 | Set 0104 | 1.00 | 392.96 | 392.96 |
| 8 | Set 0105 | 3.00 | 245.39 | 736.17 |
| 10 | Set 0106 | 1.00 | 259.56 | 259.56 |
| 12 | Set 0107 | 2.00 | 924.26 | 1,848.52 |
| 14 | Set 0108 | 1.00 | 1,727.21 | 1,727.21 |
| 16 | Set 0109 | 1.00 | 734.20 | 734.20 |
| 18 | Set 0110 | 1.00 | 1,467.60 | 1,467.60 |
| 20 | Set 0111 | 1.00 | 655.42 | 655.42 |
| 22 | Set 0112 | 1.00 | 754.82 | 754.82 |
| 24 | Set 0113 | 1.00 | 840.38 | 840.38 |
| 27 | Set 0114 | 2.00 | 429.01 | 858.02 |
| 29 | Set 0115 | 1.00 | 1,101.12 | 1,101.12 |
| 31 | Set 0116 | 1.00 | 563.76 | 563.76 |
| 33 | Set 0117 | 1.00 | 488.91 | 488.91 |
| 35 | Set 0118 | 1.00 | 367.77 | 367.77 |
| 37 | Set 0119 | 1.00 | 679.72 | 679.72 |
| 39 | Set 0120 | 1.00 | 263.51 | 263.51 |
| 41 | Set 0121 | 1.00 | 670.88 | 670.88 |
| 43 | Set 0122 | 2.00 | 125.53 | 251.06 |
| 44 | Set 0123 | 1.00 | 529.35 | 529.35 |
| 46 | Set 0124 | 1.00 | 632.36 | 632.36 |
| 48 | Set 0125 | 1.00 | 257.84 | 257.84 |
| 49 | Set 0126 | 1.00 | 332.40 | 332.40 |
| 50 | Set 0127 | 1.00 | 332.40 | 332.40 |
| 51 | Set 0128 | 2.00 | 300.25 | 600.50 |
| 53 | Set 0129 | 1.00 | 319.81 | 319.81 |
| 55 | Set 0130 | 2.00 | 270.48 | 540.96 |
| 57 | Set 0131 | 2.00 | 627.53 | 1,255.06 |
| 59 | Set 02 | 2.00 | 969.48 | 1,938.96 |
| 61 | Set 03 | 1.00 | 2,680.45 | 2,680.45 |
| 63 | Set 04 | 2.00 | 535.20 | 1,070.40 |
| 65 | Set 05 | 1.00 | 794.84 | 794.84 |
| 68 | Set 06 | 2.00 | 614.04 | 1,228.08 |
| 70 | Set 07 | 1.00 | 798.37 | 798.37 |
| 73 | Set 08 | 4.00 | 679.16 | 2,716.64 |
| 75 | Set 12 | 1.00 | 466.25 | 466.25 |
| 77 | Set 15 | 1.00 | 1,003.11 | 1,003.11 |
| 79 | Set 17 | 2.00 | 414.50 | 829.00 |
| 80 | Set 18 | 1.00 | 456.79 | 456.79 |
| 82 | Set 19 | 1.00 | 427.12 | 427.12 |
| 84 | Set 20 | 4.00 | 454.62 | 1,818.48 |
| 86 | Set 21 | 1.00 | 459.06 | 459.06 |
| 88 | Set 22 | 1.00 | 1,174.30 | 1,174.30 |
| 91 | Set 23 | 2.00 | 1,197.70 | 2,395.40 |
| 94 | Set 24 | 1.00 | 1,197.62 | 1,197.62 |
| 97 | Set 25 | 2.00 | 769.10 | 1,538.20 |
| 99 | Set 26 | 6.00 | 749.17 | 4,495.02 |
| 101 | Set 27 | 7.00 | 743.60 | 5,205.20 |
| 103 | Set 28 | 1.00 | 543.16 | 543.16 |
| 104 | Set 29 | 6.00 | 431.64 | 2,589.84 |
| 106 | Set 30 | 2.00 | 975.07 | 1,950.14 |
| 108 | Set 31 | 2.00 | 660.99 | 1,321.98 |
| 110 | Set 35 | 1.00 | 192.84 | 192.84 |
| 111 | Set 37 | 1.00 | 195.42 | 195.42 |
| 113 | Set 38 | 1.00 | 195.42 | 195.42 |
| 115 | Set 41 | 2.00 | 496.75 | 993.50 |
| 117 | Set 42 | 1.00 | 382.62 | 382.62 |
| 119 | Set 44 | 1.00 | 747.05 | 747.05 |
| 122 | Set 45 | 2.00 | 1,144.79 | 2,289.58 |
| 124 | Set 46 | 1.00 | 1,141.40 | 1,141.40 |
| 126 | Set 47 | 1.00 | 1,017.00 | 1,017.00 |
| 128 | Set 48 | 1.00 | 655.84 | 655.84 |
| 130 | Set 50 | 1.00 | 492.30 | 492.30 |
| 132 | Set 51 | 1.00 | 559.41 | 559.41 |
| 134 | Set 52 | 1.00 | 467.16 | 467.16 |
| 136 | Set 53 | 2.00 | 470.80 | 941.60 |
| 137 | Set 55 | 2.00 | 328.95 | 657.90 |
| 138 | Set 56 | 1.00 | 306.84 | 306.84 |
| 140 | Set 57 | 1.00 | 262.95 | 262.95 |
| 142 | Set 59 | 1.00 | 393.25 | 393.25 |
| 143 | Set 60 | 1.00 | 694.91 | 694.91 |
| 145 | Set 61 | 1.00 | 407.42 | 407.42 |
| 147 | Set 62 | 1.00 | 633.31 | 633.31 |
| 149 | Set 63 | 1.00 | 494.73 | 494.73 |
| 151 | Set 64 | 3.00 | 139.23 | 417.69 |
| 152 | Set 65 | 1.00 | 492.30 | 492.30 |
| 154 | Set 66 | 1.00 | 1,252.01 | 1,252.01 |
| 156 | Set 67 | 1.00 | 361.10 | 361.10 |
| 158 | Set 70 | 1.00 | 195.42 | 195.42 |
| 160 | Set 71 | 1.00 | 2,796.55 | 2,796.55 |
| 163 | Set 72 | 2.00 | 803.88 | 1,607.76 |
| 166 | Set 73 | 1.00 | 2,322.40 | 2,322.40 |
| 168 | Set 74 | 1.00 | 2,316.83 | 2,316.83 |
| 170 | Set 75 | 1.00 | 1,670.76 | 1,670.76 |
| 172 | Set 76 | 1.00 | 734.79 | 734.79 |
| 175 | Set 79 | 2.00 | 297.97 | 595.94 |
| 177 | Set 80 | 1.00 | 464.53 | 464.53 |
| 179 | Set 81 | 1.00 | 431.64 | 431.64 |
| 181 | Set 82 | 1.00 | 419.18 | 419.18 |
| 183 | Set 83 | 1.00 | 243.05 | 243.05 |
| 185 | Set 84 | 1.00 | 453.49 | 453.49 |
| 187 | Set 85 | 1.00 | 885.19 | 885.19 |
| 190 | Set 86 | 1.00 | 1,736.25 | 1,736.25 |
| 192 | Set 87 | 1.00 | 1,289.46 | 1,289.46 |
| 194 | Set 88 | 2.00 | 772.49 | 1,544.98 |
| 196 | Set 89 | 1.00 | 443.30 | 443.30 |
| 198 | Set 90 | 1.00 | 426.07 | 426.07 |
| 200 | Set 91 | 1.00 | 431.72 | 431.72 |
| 202 | Set 92 | 1.00 | 655.42 | 655.42 |
| 204 | Set 93 | 1.00 | 667.08 | 667.08 |
| 206 | Sundries | 1.00 | 293.62 | 293.62 |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | \_\_\_\_\_  151.00 | \_\_\_\_\_\_\_  Total GBP: 100,767.22 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Page** | **Door number** | **HWSet number** | **Page** | **Door number** | **HWSet number** |
|  |  |  |  |  |  |
| 206 | misc | Sundries | 22 | PM.DR.00.045A.01 | Set 0112 |
| 24 | PM.DR.00.045A.02 | Set 0113 | 46 | PM.DR.00.07b.01 | Set 0124 |
| 50 | PM.DR.00.13.01 | Set 0127 | 49 | PM.DR.00.14.05 | Set 0126 |
| 75 | PM.DR.00.16.01 | Set 12 | 103 | PM.DR.00.22.03 | Set 28 |
| 200 | PM.DR.00.25.01 | Set 91 | 128 | PM.DR.00.30A.01 | Set 48 |
| 43 | PM.DR.00.31.01 | Set 0122 | 44 | PM.DR.00.32.01 | Set 0123 |
| 110 | PM.DR.00.33.01 | Set 35 | 63 | PM.DR.00.34.01 | Set 04 |
| 63 | PM.DR.00.36.01 | Set 04 | 43 | PM.DR.00.41.02 | Set 0122 |
| 175 | PM.DR.00.44B.01 | Set 79 | 115 | PM.DR.00.46.01 | Set 41 |
| 48 | PM.DR.00.54.01 | Set 0125 | 117 | PM.DR.00.57.01 | Set 42 |
| 151 | PM.DR.00.58.01 | Set 64 | 151 | PM.DR.00.58.02 | Set 64 |
| 151 | PM.DR.00.58.03 | Set 64 | 31 | PM.DR.00.58.04 | Set 0116 |
| 115 | PM.DR.00.59.01 | Set 41 | 175 | PM.DR.00.61.01 | Set 79 |
| 126 | PM.DR.00.ST06.01 | Set 47 | 18 | PM.DR.00.ST10.01 | Set 0110 |
| 134 | PM.DR.01.04.01 | Set 52 | 51 | PM.DR.01.06.06 | Set 0128 |
| 27 | PM.DR.01.08.02 | Set 0114 | 27 | PM.DR.01.08.03 | Set 0114 |
| 149 | PM.DR.01.14.01 | Set 63 | 136 | PM.DR.01.15.01 | Set 53 |
| 16 | PM.DR.01.16.01 | Set 0109 | 136 | PM.DR.01.18.01 | Set 53 |
| 57 | PM.DR.01.18b.01 | Set 0131 | 53 | PM.DR.01.24.01 | Set 0129 |
| 55 | PM.DR.01.25.01 | Set 0130 | 55 | PM.DR.01.26.01 | Set 0130 |
| 8 | PM.DR.01.28.02 | Set 0105 | 57 | PM.DR.01.33.01 | Set 0131 |
| 140 | PM.DR.01.34.01 | Set 57 | 145 | PM.DR.01.39.01 | Set 61 |
| 130 | PM.DR.01.39.02 | Set 50 | 132 | PM.DR.01.40.03 | Set 51 |
| 147 | PM.DR.01.41B.01 | Set 62 | 33 | PM.DR.01.42.01 | Set 0117 |
| 137 | PM.DR.01.43.01 | Set 55 | 137 | PM.DR.01.44.01 | Set 55 |
| 12 | PM.DR.01.46.01 | Set 0107 | 143 | PM.DR.01.46A.02 | Set 60 |
| 142 | PM.DR.01.46B.02 | Set 59 | 12 | PM.DR.01.47.01 | Set 0107 |
| 8 | PM.DR.01.53.01 | Set 0105 | 8 | PM.DR.01.54.02 | Set 0105 |
| 156 | PM.DR.01.55.01 | Set 67 | 6 | PM.DR.01.57.01 | Set 0104 |
| 51 | PM.DR.01.59.01 | Set 0128 | 10 | PM.DR.01.62.01 | Set 0106 |
| 138 | PM.DR.01.LT3.01 | Set 56 | 124 | PM.DR.01.ST.11 | Set 46 |
| 122 | PM.DR.01.ST05.01 | Set 45 | 122 | PM.DR.01.ST10.01 | Set 45 |
| 152 | PM.DR.01.ST12.01 | Set 65 | 179 | PM.DR.B1.04.01 | Set 81 |
| 88 | PM.DR.B1.07.01 | Set 22 | 91 | PM.DR.B1.07.02 | Set 23 |
| 91 | PM.DR.B1.07.03 | Set 23 | 187 | PM.DR.B1.07.04 | Set 85 |
| 160 | PM.DR.B1.10.01 | Set 71 | 190 | PM.DR.B1.22.01 | Set 86 |
| 181 | PM.DR.B1.23.01 | Set 82 | 37 | PM.DR.B1.24.01 | Set 0119 |
| 35 | PM.DR.B1.25.01 | Set 0118 | 111 | PM.DR.B1.26.01 | Set 37 |
| 113 | PM.DR.B1.27.04 | Set 38 | 158 | PM.DR.B1.28.01 | Set 70 |
| 39 | PM.DR.B1.28.03A | Set 0120 | 183 | PM.DR.B1.30.01 | Set 83 |
| 163 | PM.DR.B1.31.01 | Set 72 | 99 | PM.DR.B1.31.02 | Set 26 |
| 68 | PM.DR.B1.33.01 | Set 06 | 68 | PM.DR.B1.34.01 | Set 06 |
| 79 | PM.DR.B1.37.01 | Set 17 | 61 | PM.DR.B1.38.01 | Set 03 |
| 4 | PM.DR.B1.39.01 | Set 01 | 172 | PM.DR.B1.40.01 | Set 76 |
| 80 | PM.DR.B1.41.01 | Set 18 | 59 | PM.DR.B1.43.01 | Set 02 |
| 106 | PM.DR.B1.44.01 | Set 30 | 106 | PM.DR.B1.45.01 | Set 30 |
| 84 | PM.DR.B1.46.01 | Set 20 | 84 | PM.DR.B1.47.01 | Set 20 |
| 84 | PM.DR.B1.48.01 | Set 20 | 84 | PM.DR.B1.49.01 | Set 20 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Page** | **Door number** | **HWSet number** | **Page** | **Door number** | **HWSet number** |
|  |  |  |  |  |  |
| 86 | PM.DR.B1.51.01 | Set 21 | 4 | PM.DR.B1.52.01 | Set 01 |
| 99 | PM.DR.B1.53.01 | Set 26 | 194 | PM.DR.B1.54.01 | Set 88 |
| 192 | PM.DR.B1.58.03 | Set 87 | 14 | PM.DR.B1.58.04 | Set 0108 |
| 29 | PM.DR.B1.PL02.01 | Set 0115 | 99 | PM.DR.B1.PL03A.01 | Set 26 |
| 194 | PM.DR.B1.PL03A.02 | Set 88 | 101 | PM.DR.B1.PL04.01 | Set 27 |
| 77 | PM.DR.B1.PL06.01 | Set 15 | 4 | PM.DR.B1.PL07.01 | Set 01 |
| 99 | PM.DR.B1.PL08.01 | Set 26 | 99 | PM.DR.B1.PL09.01 | Set 26 |
| 177 | PM.DR.B1.PL10.01 | Set 80 | 119 | PM.DR.B1.PL11.01 | Set 44 |
| 101 | PM.DR.B1.PL13.01 | Set 27 | 101 | PM.DR.B1.PL14.01 | Set 27 |
| 99 | PM.DR.B1.PL15.01 | Set 26 | 185 | PM.DR.B1.PL16.01 | Set 84 |
| 101 | PM.DR.B1.PL18.01 | Set 27 | 101 | PM.DR.B1.PL19.01 | Set 27 |
| 101 | PM.DR.B1.PL20.01 | Set 27 | 104 | PM.DR.B1.PL22.01 | Set 29 |
| 101 | PM.DR.B1.PL22.02 | Set 27 | 20 | PM.DR.B1.PL23.01 | Set 0111 |
| 59 | PM.DR.B1.SCR01.01 | Set 02 | 154 | PM.DR.B1.ST05.01 | Set 66 |
| 82 | PM.DR.B1.ST05.02 | Set 19 | 104 | PM.DR.B1.ST06.01 | Set 29 |
| 170 | PM.DR.B1.ST06.02 | Set 75 | 168 | PM.DR.B1.ST10.01 | Set 74 |
| 166 | PM.DR.B1.ST11.01 | Set 73 | 196 | PM.DR.BM.01.01 | Set 89 |
| 65 | PM.DR.BM.02.01 | Set 05 | 202 | PM.DR.BM.04.01 | Set 92 |
| 104 | PM.DR.BM.05.01 | Set 29 | 41 | PM.DR.BM.06.01 | Set 0121 |
| 204 | PM.DR.BM.08.01 | Set 93 | 104 | PM.DR.BM.09.01 | Set 29 |
| 94 | PM.DR.BM.10.01 | Set 24 | 73 | PM.DR.BM.11A.01 | Set 08 |
| 73 | PM.DR.BM.11A.02 | Set 08 | 73 | PM.DR.BM.13.01 | Set 08 |
| 97 | PM.DR.BM.14.01 | Set 25 | 70 | PM.DR.BM.14.02 | Set 07 |
| 97 | PM.DR.BM.15.01 | Set 25 | 104 | PM.DR.BM.16.01 | Set 29 |
| 198 | PM.DR.BM.18.01 | Set 90 | 163 | PM.DR.BM.19.01 | Set 72 |
| 73 | PM.DR.BM.PL01 | Set 08 | 79 | PM.DR.BM.SCR02.01 | Set 17 |
| 104 | PM.DR.BM.SCR03.02 | Set 29 | 108 | PM.DR.BM.SCR07.01 | Set 31 |
| 108 | PM.DR.BM.ST05.01 | Set 31 | 0 |  |  |

|  |  |  |
| --- | --- | --- |
| Terms and Conditions  1. General.  1.1 In these terms and conditions:  (a) "Company" means Allgood Ltd its subsidiaries and agents  (b) "Goods" means the articles equipments and/or services to which this document relates and  (c) "Buyer" means the purchaser of Goods from the Company.  1.2 All orders are accepted and Goods supplied by the Company subject to these terms and conditions and except insofar as any exclusion or restriction of liability may be prohibited by statute all other conditions warranties and representations express or implied and statutory or otherwise except as to title are hereby excluded. No addition thereto or variation therefrom whether contained in the Buyer's order or otherwise  shall apply unless agreed in writing by the Company.  2. Orders, Cancellations, Deliveries and Returns  2.1 All orders are subject to availability of Goods and to written acceptance by the Company on its acceptance of order form for the time being in use any prior acceptance by the Company being provisional only. The Company reserves the right (without prejudice to any other remedy) to cancel any uncompleted order or to suspend delivery in the event of any of the Buyer's commitments to the Company not being met.  2.2 Cancellation of any order or part thereof or rescheduling of deliveries by the Buyer will only be considered by the Company if made in writing. If any order is cancelled or rescheduled by the Company in the aforesaid circumstances or is cancelled or rescheduled by the Buyer then the Buyer shall indemnify the Company against all loss costs (including the cost of all labour and materials used and overheads incurred) damages charges and expenses arising out of the order and the cancellation or rescheduling thereof without prejudice to any other rights of the Company.  2.3 The Company may at its sole discretion accept returns of unwanted Goods.  Goods will only be considered for return if in the original undamaged and unopened packaging and will be subject to a re-stocking charge.  3. Prices  3.1 Except in respect of where the price is expressly stated to be fixed for a specific delivery period the Company reserves its right to alter its quotation or order prices in respect of the Goods by reference to the price ruling at the date of despatch of the Goods by any additional sum as may from time to time be necessary to cover increases in the costs of the materials and / or labour (or any other factor affecting the cost of production or delivery) which may occur between the date of contract and the date of despatch.  3.2 Where in a quotation or acceptance of order a price is expressly fixed for a specific delivery period and for any reason (except where the same is due to the fault of the Company) a supply is made under the quotation or order after the end of the said period the Company reserves the right in respect of such supply to charge the price ruling at the date of despatch of the Goods in like manner as in condition 3.1  above.  3.3 A quotation of the Company does not constitute an offer by the Company to supply the Goods and every acceptance of any quotation of the Company and every order by the Buyer in response to any quotation of the Company shall be deemed an offer by the Buyer to the Company and will not be binding on the Company until the Company has given its written confirmation of acceptance of such order.  3.4 A quotation which is stated to be for a fixed price shall be deemed to have been withdrawn in any event unless an order in respect thereof is placed for delivery within the period specified in the quotation.  4. Delivery  4.1 Where a quotation or acceptance of order specifies a delivery period but the Company is unable to complete delivery without further information of details from the Buyer and there is in the opinion of the Company a delay on the part of the Buyer in providing the information or details then the Company may if it wishes give notice extending the delivery period and without prejudice to the Company's rights to vary its prices under Condition 3 hereof.  4.2 Any date or period set out therein for the delivery of the Goods or any part of them shall not be of the essence of the contract and if the Company is prevented from delivering any Goods at the time provided for delivery by reasons of any cause outside its reasonable control including but not so as to limit the generality of the foregoing fire explosion plant breakdown interference by labour strikes or lockouts or nonavailability of transport or materials then the period for delivery shall be extended to such extent as shall be reasonable having regard to the circumstances.  5. Carriage  5.1 All prices stated or referred to in the Company's quotation or in the Company's acceptance of order exclude any carriage or packing charges which shall be paid by the Buyer.  5.2 Where prices are quoted inclusive of delivery, this allows for one “anytime next day” delivery and not for a specific timed slot nor any non-standard delivery requirements. (These are available on request and at an extra charge depending upon requirements). Applies to mainland UK only, delivery to all others region will be priced upon request.  6. Warranties and Claims  6.1 The Company will make every endeavour to supply goods suitable to the Buyer's requirements and accordingly if the Goods after inspection by the Company or its agents are accepted by the Company by reason of faulty material or workmanship as being unmerchantable at the time of supply or unfit for any specific purpose which has been made known to the Company prior to the making of the contract or as differing materially from their description or from any sample supplied the Company undertakes to replace such Goods or (at the option of the Company) to refund the purchase price or a fair proportion thereof. This undertaking by the Company is subject to and conditional upon the following provisions.  6.2 The Buyer must give notice in writing to the Company of any claim within 12 months of receipt of the Goods and within 14 days after the discovery of the complaint.  6.3 Such replacement or refund by the Company shall be the absolute limit of the Company's liability to the Buyer in respect of any such Goods and any further claims including claims for consequential loss and damages are excluded.  6.4 Whilst the Company warrants that any survey advice representation schedule or forecast given on the part of the Company from anything said or written in discussions or negotiations between the Company and the Buyer or their respective agents or by the Company to any other parties prior to the making of the contract is given in good faith and after due consideration of the facts before the Company the Company shall be under no legal liability whether in negligence or howsoever in respect thereof to the Buyer or any other person except to the extent to which there is a breach of this warranty.  6.5 No claim can be entertained for Goods short delivered or damaged in transit unless either (where this is possible) a receipt is given to the carrier detailing the shortage or damage at the time of delivery or notification of the shortage or damage is made to the Company within seven days from the delivery of Goods by the carrier.  6.6 No claim for non-delivery of the Goods can be entertained unless the Company is notified in writing within seven days from the date of its invoice for the said Goods.  6.7 Any guarantee or warranty for the Goods is subject to (a) the Company having received full payment for the Goods and (b) the Goods having been maintained and serviced in accordance with the manufacturer’s recommendations and/or maintenance requirements.  7. Passing of risk  7.1 The risk in the Goods shall pass to the Buyer when the Company delivers the Goods in accordance with the terms hereof to the Buyer or other person to whom the Company has been authorised by the Buyer to deliver the Goods whether expressly or by implication and the Company shall not be liable for the protection of the Goods thereafter and the Buyer shall insure and protect the Goods thereafter against such risk as may be commercially prudent.  8. Payment  8.1 Unless otherwise specifically agreed all invoices are payable against Proforma invoice or by a recognised Credit Card. All prices quoted are exclusive of Value Added Tax unless otherwise stated in writing and the Buyer shall in addition to the price of the Goods pay any Value Added Tax which may be payable. | 8.2 If the Company agrees to allow the Buyer credit the Company may at any time at its sole discretion limit or cancel such credit and may require payment of all or any part of contract price for the Goods to be made in cash in advance of delivery or may require guarantees or other security to be provided and any payment or security so required shall be paid or furnished by the Buyer promptly upon such requirement being notified to the Buyer. The Company shall be under no obligation to deliver the Goods or any part thereof unless and until the Buyer has complied with this condition and has discharged all its other obligations to the Company under the order and on any other account.  8.3 All Goods supplied on credit shall be paid for within 30 days from the end of the calendar month in which they are invoiced by the Company. If any settlement discount is offered by the Company then the same shall be deductible only if the Goods are paid for within the said period of 30 days and on no account shall discount be deductible from the Value Added Tax.  8.4 Payment of an account in full by the due date shall be a condition precedent to future deliveries under the same or any other contracts existing between the Company and the Buyer and the Company may suspend delivery thereof until this condition is satisfied.  8.5 If the Buyer fails to make payments for Goods supplied as aforesaid then without prejudice to any other rights the Company may have, the Company shall be entitled to exercise its statutory rights to claim interest and compensation for debt recovery costs under the current late payment legislation.  9. Property in Goods  9.1 Until payment by the Buyer in full of the price and any other monies payable to the Company in respect of Goods:-  (a) Property in the Goods shall remain with the Company.  (b) The Buyer shall hold the Goods as bailee for the Company and shall so store and protect them so that they shall at all times be identifiable as Goods of the Company provided that the Buyer may until the occurrence of any of the events specified in condition 9 below sell process or otherwise dispose of or deal with the Goods in ordinary course of its business.  10. Buyer's Default  10.1 If the Buyer shall default in or commit breach of any of its obligations to the Company or if the Buyer (or when the Buyer is a firm any partner in that firm) shall at any time become bankrupt or shall have a receiving order or administration order made against him or shall make any composition or arrangement with or for the benefit of his creditors or shall make any conveyance or assignment for the benefit of his creditors or shall purport to do so or any application shall be made under any bankruptcy act for the time being in force for sequestration of his estate or a trust deed shall be granted by him on behalf of his creditors or the Buyer being an incorporated body if any resolution or petition to wind up its business shall be passed or presented otherwise than for reconstruction or amalgamation or if a receiver or manager of the Buyer's undertaking property or assets or any part thereof shall be appointed or if the Buyer shall be insolvent or shall be unable or be deemed unable or shall admit its inability to meet its commitments promptly as and when due or if any other event shall occur which in the Company's opinion gives ground for believing that the Buyer's ability to perform its obligations under any order may be impaired then and in any such event or the equivalent thereof in the Buyer's country of domicile the company may (without prejudice to any other right or remedy which it might have):  (a) forthwith determine all or any orders in whole or in part by notice in writing;  and/or  (b) repossess any of the Goods held by the Buyer in which property has not yet passed to the Buyer and for this purpose enter upon any premises of the Buyer and sever the same from any assets of the Buyer; and/or  (c) forthwith demand immediate payment of the contract price of the Goods and all other sums which may be outstanding to the Company on any account whereupon the same shall become immediately due and payable; and/or  (d) resell all or any of the Goods without further notice to the Buyer upon such terms and conditions as the Company may in its discretion determine.  11. Design  11.1 The Company reserves the right to alter modify or improve the design of any Goods without notification and Buyer’s orders will be executed with current production. This may include (but shall not be limited to) plated or applied finishes that the Company may at its discretion deem appropriate and such finishes shall be deemed of acceptable visual quality if, when the Goods are installed, they display no defects visible by the naked eye at a distance of a metre away.  11.2 Where Goods are ordered in accordance with the designs drawings and specifications or samples furnished by the Buyer or compiled on behalf and approved by the Buyer the Buyer shall indemnify the Company against all liability or alleged liability in respect of any infringement of intellectual property rights of third parties arising out of the manufacture sale or use of such Goods and against all claims demands proceedings damage costs and expenses arising in respect of such liability or alleged liability.  12. Installation and site works  12.1 Any reference to "Installation" only refers to quotations where installation has been expressly stated to be included in a hardware set and only refers to hardwired doors. All other doors and Goods are to be fitted by others, unless otherwise stated.  12.2 All prices quoted are subject to confirmation following receipt of full door and frame details and full site survey. If as a result of the survey or on receipt of full details additional equipment is required additional charges will be made. It is the responsibility of the Buyer to ensure that all information is made available to the Company at the appropriate time.  12.3 All prices quoted are on the basis that the Company will be permitted continuous and uninterrupted working and full, unrestricted access to all areas during the installation and are based on site works being carried out in one continuous visit during normal working hours between Monday and Friday only.  12.4 In the event of any delay or disruption to the installation works the Company shall be entitled to reasonable extension of time for completion and the extra cost of any weekend shift out of hours working return visit or waiting time caused by or executed at request of the Buyer or to rectify delays caused by the Buyer shall be added to the price at the Company's surcharge rate plus any additional travel costs.  12.5 Preparatory and other work to be carried out and goods to be supplied and/or services or attendances to be provided by the Buyer its servants or agents or by third parties shall be executed to the Company's satisfaction  Delivery and Installation  12.6 All Delivery and/or installation times and periods are estimates only and will be confirmed upon receipt of order and all necessary manufacturing details.  12.7 Following receipt of an order, the Company requires notice in writing from the Buyer a minimum of 4 weeks before commencement of installation to allow works to be scheduled.  12.8 For installation the Company must be contacted at time of electrical first fix to enable containment details to be discussed.  12.9 Not less than 5 working days before commencement of the installation the Buyer shall provide to the Company a signed Site Ready Sheet. The Company reserves the right not to attend site until a signed Site Ready Sheet has been provided and notice has been given under condition 11.7 above.  12.10 The Buyer is to provide vehicular access and parking on site free of charge. Any additional costs incurred by the Company for parking will be passed on as an additional charge.  12.11 In the event that the Company is not permitted to complete the commissioning and demonstration of the system in the same visit as the installation the cost of returning to site to complete the commissioning and/or demonstration at a later date will be an additional charge.  12.12 Until the commissioning and demonstration has been completed the equipment must not be used and the system should be immobilised to prevent it being operated. No liability will be accepted for loss or damage caused to the Goods or injury to persons by unauthorised use. Call-outs to site due to misuse or vandalism will be chargeable.  Warranty  12.13 Electrical door products carry a twelve month warranty other than where damage is caused by misuse abuse lack of maintenance or adjustment of the door.  Electrical Requirements | 12.14 The Buyer shall provide the following facilities free of charge:-  a) Connection to a fire alarm system (if required) will require 1 pair of normally open volt free contacts with optional relay contacts to be supplied terminating at each drive unit location by the Fire Alarm Contractor.  b) Any concealed containment (inc. draw wires). Cabling to activation devices will be otherwise fitted by the Company in white plastic surface mini trunking at a distance deemed to be reasonable by the Company.  c) Where access controls or locking mechanisms are to be supplied by others, the Buyer must provide a clearly marked pair of contacts adjacent to the control unit to allow final connection at the time of installation. If the Company is required toundertake additional control cabling to these devices or additional visits then extra charges will be levied.  d) 1no. live 240volt 5amp switched fused spur to each opening leaf positioned within 1 metre above the door operator location subject to site conditions.  e) Power to the fused spur, at the time of installation, to allow set up, test and commissioning of equipment.  Builders Work  12.15 The price quoted is based on installation by the Company within a prepared structural opening with finished floor level in position prior to our agreed site commencement date. Openings must be true and plumb to allow commissioning of door leaves. An adequate solid vertical surface, above the door, for fixing our automatic opening equipment must be provided and builder’s work details can be supplied by the Company if requested.  12.16 Where the quotation includes Second Fix and Commissioning of the specified equipment all containment drilling and cutting into doors and/or frames shall be completed by others free of charge. The Company will take reasonable steps to avoid causing damage to door frames walls and the like but all making good and redecorating will be carried out by others at no cost to the Company.  12.17 The Buyer shall be responsible without charge to the Company for:  (i) off-loading;  (ii) provision maintenance erection and dismantling of any necessary scaffolding staging towers access equipment etc and provision of any necessary mobile cranes hoists and the like and should it be a requirement for the Company to provide any Working at Height equipment then extra charges will be levied.  (iii) builder’s or civil work including excavation cutting away and making good including to any damage to decorative finishes in the work area and any decoration required after installation;  (iv) any removal dismantling and reinstatement of existing structure and equipment including doors frames and screens and removal of any redundant items etc from the job site;  (v) provision of power light fire fighting equipment temporary screen or enclosures first aid facilities site huts store huts messing facilities toilets etc;  (vi) connections of main services to the installed goods;  (vii) waiting time multiple visits to site and interrupted working by other trades;  (viii) providing an adequate facility to the Company for indoor storage of Goods in close proximity to installation area.  Set-up and Training  12.18 Prices for Set-up and Training are based on a single visit for both Set Up of and Training for the Access Control system. Training will be carried out during the system Set-Up stage. Should this not be possible an additional charge will be levied for subsequent days.  12.19 All equipment must be installed and operating on factory default and software and programming devices must be available prior to Training commencing.  12.20 For computer based systems the Buyer must provide a computer for the Company’s use to enable to installation of software and subsequent programming of equipment.  12.21 All relevant information must be provided by the Buyer at time of system Set- Up to enable a fully operational system. Information required will include Names, Access Levels, Time Periods and the like.  12.22 In the event that the Company is required to change the system from factory default to a unique default, in advance of the full Set-Up of the system, an additional charge will be levied.  12.23 If the Buyer requires databases to be installed on its IT network then an appropriate IT representative of the Buyer must be present.  12.24 The Company cannot accept liability should any conflict of programmes occur on a Buyer’s computer.  Safety Information  12.25 To comply with Health and Safety requirements it may be necessary for the Buyer to provide an alternative means of entry / exit to the building to be used whilst work is being carried out.  12.26 The Company will supply door safety signage in respect of the installation work. The Company accepts no liability for any loss damage or injury that may occur as a result of the unauthorised removal of door signage by others.  12.27 For automatic doors, the Buyer must ensure that on completion of the installation, daily safety and operational checks are carried out by suitably trained personnel.  12.28 The Buyer must also ensure that periodic safety checks are carried out to nsure that the equipment remains in good working order.  Additional Requirements  12.29 In the event that the Company’s operatives are required to attend a Site Induction course of more than 1 hour additional charges may be levied.  12.30 Any plant or equipment provided by the Company in relation to the performance of the Company's obligations is provided exclusively for the use of the Company or its agents or employees and any other persons using such plant or equipment do so at the Buyer's risk. The Buyer indemnifies the Company against any claim made against the Company in respect of the use of such plant or equipment and for making good any damage so caused.  13. Limitation of liability  13.1 It is expressly stipulated that in the event of any claim on any ground being made by the Buyer against the Company in respect of the Goods or any matter arising from or in relation to the order relating thereto the liability of the Company shall be limited (in respect of each claim or series of connected claims) to the invoice value of the Goods and under no circumstances shall the Company be liable for loss of profit or any consequential loss howsoever arising.  13.2 In the event that any provision of these Terms and Conditions are deemed invalid or unenforceable in any jurisdiction, all other provisions will remain in full force and effect and the affected provision will be modified only to the extent of such invalidity or unenforceability in that jurisdiction and shall otherwise remain in full force and effect. These Terms and Conditions will remain in full force and effect in any jurisdiction without such restriction.  14. Data Protection  14.1 By submitting information to the Company, the Buyer (and each individual as applicable) consents to such information being processed by the Company in accordance with the Data Protection Act 1998 ("DPA").  14.2 The Buyer consents to the Company using such information as follows:-  (a) To supply Goods as requested by the Buyer including such transfer of the information to employees, agents and third parties as required for this purpose;  (b) For the Company’s internal administration purposes including the transfer between departments divisions of companies within the Company;  (c) To market the Company’s Goods to the Buyer (and each individual as applicable);  (d) To transfer ownership of the information on sale or merger of all or any part of the Company;  (e) To process the information to obtain legal advice, comply with legal requirements protect the Company’s rights and property and the safety of the Company’s employees clients suppliers and others.  15. Law Applicable  15.1 Each order and these terms and conditions shall be governed by and constructed in all respects in accordance with the laws of England.  16. Waiver  16.1 Failure or delay by the Company to enforce any of its rights against the Buyer shall not be construed as a waiver of such rights.  17. Relaxation  17.1 These terms and conditions of sale enable the Company to maintain a cost effective service to the Buyer. Relaxation of any of them may be available for an agreed consideration |